3GPP TS 29.571 V16.0.0 (2019-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

5G System; Common Data Types for Service Based Interfaces;

Stage 3

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

3GPP, 5G System

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 6

1 Scope 7

2 References 7

3 Definitions and abbreviations 8

3.1 Definitions 8

3.2 Abbreviations 8

4 Overview 8

5 Common Data Types 8

5.1 Introduction 8

5.2 Data Types for Generic Usage 9

5.2.1 Introduction 9

5.2.1A Re-used Data Types 9

5.2.2 Simple Data Types 9

5.2.3 Enumerations 13

5.2.3.1 Enumeration: PatchOperation 13

5.2.3.2 Enumeration: UriScheme 14

5.2.3.3 Enumeration: ChangeType 14

5.2.4 Structured Data Types 15

5.2.4.1 Type: ProblemDetails 15

5.2.4.2 Type: Link 15

5.2.4.3 Type PatchItem 16

5.2.4.4 Type: LinksValueSchema 16

5.2.4.5 Type: SelfLink 16

5.2.4.6 Type: InvalidParam 16

5.2.4.7 Type: LinkRm 16

5.2.4.8 Type ChangeItem 17

5.2.4.9 Type NotifyItem 17

5.2.4.10 Type: ComplexQuery 17

5.2.4.11 Type: Cnf 18

5.2.4.12 Type: Dnf 18

5.2.4.13 Type: CnfUnit 18

5.2.4.14 Type: DnfUnit 18

5.2.4.15 Type: Atom 18

5.2.4.16 Type: NFDiscFactors 19

5.3 Data Types related to Subscription, Identification and Numbering 20

5.3.1 Introduction 20

5.3.2 Simple Data Types 20

5.3.3 Enumerations 23

5.3.4 Structured Data Types 23

5.3.4.1 Type: Guami 23

5.3.4.2 Type: NetworkId 23

5.3.4.3 Type: GuamiRm 23

5.4 Data Types related to 5G Network 23

5.4.1 Introduction 23

5.4.2 Simple Data Types 23

5.4.3 Enumerations 26

5.4.3.1 Enumeration: AccessType 26

5.4.3.2 Enumeration: RatType 26

5.4.3.3 Enumeration: PduSessionType 26

5.4.3.4 Enumeration: UpIntegrity 27

5.4.3.5 Enumeration: UpConfidentiality 27

5.4.3.6 Enumeration: SscMode 27

5.4.3.7 Enumeration: DnaiChangeType 27

5.4.3.8 Enumeration: RestrictionType 28

5.4.3.9 Enumeration: CoreNetworkType 28

5.4.3.10 Enumeration: AccessTypeRm 28

5.4.3.11 Enumeration: RatTypeRm 28

5.4.3.12 Enumeration: PduSessionTypeRm 28

5.4.3.13 Enumeration: UpIntegrityRm 28

5.4.3.14 Enumeration: UpConfidentialityRm 28

5.4.3.15 Enumeration: SscModeRm 28

5.4.3.17 Enumeration: DnaiChangeTypeRm 29

5.4.3.18 Enumeration: RestrictionTypeRm 29

5.4.3.19 Enumeration: CoreNetworkType 29

5.4.3.20 Enumeration: PresenceState 29

5.4.4 Structured Data Types 29

5.4.4.1 Type: SubscribedDefaultQos 29

5.4.4.2 Type: Snssai 30

5.4.4.3 Type: PlmnId 30

5.4.4.4 Type: Tai 30

5.4.4.5 Type: Ecgi 31

5.4.4.6 Type: Ncgi 31

5.4.4.7 Type: UserLocation 31

5.4.4.8 Type: EutraLocation 32

5.4.4.9 Type: NrLocation 33

5.4.4.10 Type: N3gaLocation 33

5.4.4.11 Type: UpSecurity 34

5.4.4.12 Type: NgApCause 34

5.4.4.13 Type: BackupAmfInfo 34

5.4.4.14 Type: RefToBinaryData 34

5.4.4.15 Type RouteToLocation 35

5.4.4.16 Type RouteInformation 35

5.4.4.17 Type: Area 35

5.4.4.18 Type: ServiceAreaRestriction 36

5.4.4.19 Type: PlmnIdRm 36

5.4.4.20 Type: TaiRm 36

5.4.4.21 Type: EcgiRm 36

5.4.4.22 Type: NcgiRm 36

5.4.4.23 Type: EutraLocationRm 36

5.4.4.24 Type: NrLocationRm 36

5.4.4.25 Type: UpSecurityRm 36

5.4.4.26 Type: RefToBinaryDataRm 37

5.4.4.27 Type: PresenceInfo 37

5.4.4.28 Type: GlobalRanNodeId 37

5.4.4.29 Type: GNbId 38

5.4.4.30 Type: PresenceInfoRm 38

5.4.4.31 Type: MaPduCapability 38

5.4.4.32 Type: AtsssCapability 39

5.5 Data Types related to 5G QoS 39

5.5.1 Introduction 39

5.5.2 Simple Data Types 39

5.5.3 Enumerations 42

5.5.3.1 Enumeration: PreemptionCapability 42

5.5.3.2 Enumeration: PreemptionVulnerability 42

5.5.3.3 Enumeration: ReflectiveQosAttribute 42

5.5.3.4 Void 42

5.5.3.5 Enumeration: NotificationControl 43

5.5.3.6 Enumeration: QosResourceType 43

5.5.3.7 Enumeration: PreemptionCapabilityRm 43

5.5.3.8 Enumeration: PreemptionVulnerabilityRm 43

5.5.3.9 Enumeration: ReflectiveQosAttributeRm 43

5.5.3.10 Enumeration: NotificationControlRm 43

5.5.3.11 Enumeration: QosResourceTypeRm 43

5.5.3.12 Enumeration: AdditionalQosFlowInfo 43

5.5.4 Structured Data Types 44

5.5.4.1 Type: Arp 44

5.5.4.2 Type: Ambr 44

5.5.4.3 Type: Dynamic5Qi 44

5.5.4.4 Type: NonDynamic5Qi 45

5.5.4.5 Type: ArpRm 45

5.5.4.6 Type: AmbrRm 45

5.6 Data Types related to 5G Trace 45

5.6.1 Introduction 45

5.6.2 Simple Data Types 45

5.6.3 Enumerations 45

5.6.3.1 Enumeration: TraceDepth 45

5.6.3.2 Enumeration: TraceDepthRm 46

5.6.4 Structured Data Types 47

5.6.4.1 Type: TraceData 47

5.7 Data Types related to 5G Operator Determined Barring 49

5.7.1 Introduction 49

5.7.2 Simple Data Types 49

5.7.3 Enumerations 49

5.7.3.1 Enumeration: RoamingOdb 49

5.7.4.1 Enumeration: OdbPacketServices 49

5.7.4 Structured Data Types 50

5.7.4.1 Type: OdbData 50

5.8 Data Types related to Charging 50

5.8.1 Introduction 50

5.8.2 Simple Data Types 50

5.8.3 Enumerations 50

5.8.4 Structured Data Types 50

5.8.4.1 Type: SecondaryRatUsageReport 50

5.8.4.2 Type: QoSFlowUsageReport 51

5.8.4.3 Type: SecondaryRatUsageInfo 51

5.8.4.4 Type: VolumeTimedReport 51

Annex A (normative): OpenAPI specification 51

A.1 General 51

A.2 Data related to Common Data Types 52

Annex B (informative): Change history 77

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the stage 3 protocol and data model for common data types that are used or may be expected to be used by multiple Service Based Interface APIs supported by the same or different Network Function(s).

The Principles and Guidelines for Services Definition are specified in 3GPP TS 29.501 [2].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[3] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[4] IETF RFC 1166: "Internet Numbers".

[5] IETF RFC 5952: "A recommendation for IPv6 address text representation".

[6] IETF RFC 3986: "Uniform Resource Identifier (URI): Generic Syntax".

[7] 3GPP TS 23.003: "Numbering, addressing and identification".

[8] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[9] IETF RFC 7807: "Problem Details for HTTP APIs".

[10] IETF RFC 3339: "Date and Time on the Internet: Timestamps".

[11] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP) ".

[12] IETF RFC 6901: "JavaScript Object Notation (JSON) Pointer".

[13] 3GPP TS 24.007: "Mobile radio interface signalling layer 3; General aspects".

[14] IETF RFC 6902: "JavaScript Object Notation (JSON) Patch".

[15] IETF RFC 4122: "A Universally Unique IDentifier (UUID) URN Namespace"

[16] 3GPP TS 36.413: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); S1 Application Protocol (S1AP)".

[17] IETF RFC 7042: "IANA Considerations and IETF Protocol and Documentation Usage for IEEE 802 Parameters".

[18] IETF RFC 6733: "Diameter Base Protocol".

[19] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[20] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[21] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[22] Void

[23] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[24] ITU-T Recommendation Q.763 (1999): "Specifications of Signalling System No.7; Formats and codes".

[25] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[26] 3GPP TS 23.015: "Technical Realization of Operator Determined Barring".

[27] 3GPP TR 21.900: "Technical Specification Group working methods".

[28] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[29] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core Network

DNAI Data Network Access Identifier

GPSI Generic Public Subscription Identifier

GUAMI Globally Unique AMF Identifier

PEI Permanent Equipment Identifier

SBI Service Based Interface

SUPI Subscription Permanent Identifier

# 4 Overview

For the different 5GC SBI API, data types shall be defined. Data types identified as common data types shall be defined in this Technical specification and should be referenced from individual 5GC SBI API specifications.

Data types applicable or intended to be applicable to several 5GC SBI API specifications should be interpreted as common data types.

# 5 Common Data Types

## 5.1 Introduction

In the following clauses, common data types for the following areas are defined:

- Data types for generic usage;

- Data types for Subscription, Identification and Numbering;

- Data types related to 5G Network;

- Data types related to 5G QoS;

- Data types related to 5G Trace;

- Data types related to 5G ODBs.

## 5.2 Data Types for Generic Usage

### 5.2.1 Introduction

This clause defines common data types for generic usage.

### 5.2.1A Re-used Data Types

This clause specifies the re-used data types from other specifications.

Table 5.2.1A-1: Re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data Type | Reference | Comments |
| Fqdn | 3GPP TS 29.510 [29] |  |
| NFType | 3GPP TS 29.510 [29] |  |
| ServiceName | 3GPP TS 29.510 [29] |  |
| DataSetId | 3GPP TS 29.510 [29] |  |
| PlmnSnssai | 3GPP TS 29.510 [29] |  |

### 5.2.2 Simple Data Types

This clause specifies common simple data types.

Table 5.2.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
| Binary | string | String with format "binary" as defined in OpenAPI Specification [3] |
| BinaryRm | string | This data type is defined in the same way as the "Binary" data type, but with the OpenAPI "nullable: true" property. |
| Bytes | string | String with format "byte" as defined in OpenAPI Specification [3], i.e, base64-encoded characters, |
| BytesRm | string | This data type is defined in the same way as the "Bytes" data type, but with the OpenAPI "nullable: true" property. |
| Date | string | String with format "date" as defined in OpenAPI Specification [3] |
| DateRm | string | This data type is defined in the same way as the "Date" data type, but with the OpenAPI "nullable: true" property. |
| DateTime | string | String with format "date-time" as defined in OpenAPI Specification [3] |
| DateTimeRm | string | This data type is defined in the same way as the "DateTime" data type, but with the OpenAPI "nullable: true" property. |
| DiameterIdentity | string | String containing a Diameter Identity, according to clause 4.3 of IETF RFC 6733 [18].  Pattern: '^([A-Za-z0-9]+([-A-Za-z0-9]+)\.)+[a-z]{2,}$' |
| DiameterIdentityRm | string | This data type is defined in the same way as the "DiameterIdentity" data type, but with the OpenAPI "nullable: true" property. |
| Double | number | Number with format "double" as defined in OpenAPI Specification [3] |
| DoubleRm | number | This data type is defined in the same way as the "Double" data type, but with the OpenAPI "nullable: true" property. |
| DurationSec | integer | Unsigned integer identifying a period of time in units of seconds. |
| DurationSecRm | integer | This data type is defined in the same way as the "DurationSec" data type, but with the OpenAPI "nullable: true" property. |
| Float | number | Number with format "float" as defined in OpenAPI Specification [3] |
| FloatRm | number | This data type is defined in the same way as the "Float" data type, but with the OpenAPI "nullable: true" property. |
| Uint16 | integer | Unsigned 16-bit integers, i.e. only value between 0 and 65535 are permissible. |
| Uint16Rm | integer | This data type is defined in the same way as the "Uint16" data type, but with the OpenAPI "nullable: true" property. |
| Int32 | integer | Integer with format "int32" as defined in OpenAPI Specification [3] |
| Int32Rm | integer | This data type is defined in the same way as the "Int32" data type, but with the OpenAPI "nullable: true" property. |
| Int64 | integer | Integer with format "int64" as defined in OpenAPI Specification [3] |
| Int64Rm | integer | This data type is defined in the same way as the "Int64" data type, but with the OpenAPI "nullable: true" property. |
| Ipv4Addr | string | String identifying a IPv4 address formatted in the "dotted decimal" notation as defined in in IETF RFC 1166 [4].  Pattern: '^(([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])$' |
| Ipv4AddrRm | string | This data type is defined in the same way as the "Ipv4Addr" data type, but with the OpenAPI "nullable: true" property. |
| Ipv6Addr | string | String identifying an IPv6 address formatted according to clause 4 of IETF RFC 5952 [5]. The mixed IPv4 IPv6 notation according to clause 5 of IETF RFC 5952 [5] shall not be used.  Pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))$'  and  Pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))$' |
| Ipv6AddrRm | string | This data type is defined in the same way as the "Ipv6Addr" data type, but with the OpenAPI "nullable: true" property. |
| Ipv6Prefix | string | String identifying an IPv6 address prefix formatted according to clause 4 of IETF RFC 5952 [5].  Pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))(\/(([0-9])|([0-9]{2})|(1[0-1][0-9])|(12[0-8])))$'  and  Pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))(\/.+)$' |
| Ipv6PrefixRm | string | This data type is defined in the same way as the "Ipv6Prefix" data type, but with the OpenAPI "nullable: true" property. |
| MacAddr48 | string | String identifying a MAC address formatted in the hexadecimal notation according to clause 1.1 and clause 2.1 of IETF RFC 7042 [17].  Pattern: '^([0-9a-fA-F]{2})((-[0-9a-fA-F]{2}){5})$' |
| MacAddr48Rm | string | This data type is defined in the same way as the "MacAddr48" data type, but with the OpenAPI "nullable: true" property. |
| SupportedFeatures | string | A string used to indicate the features supported by an API that is used as defined in clause 6.6 in 3GPP TS 29.500 [25]. The string shall contain a bitmask indicating supported features in hexadecimal representation:  Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent the support of 4 features as described in table 5.2.2-3. The most significant character representing the highest-numbered features shall appear first in the string, and the character representing features 1 to 4 shall appear last in the string. The list of features and their numbering (starting with 1) are defined separately for each API. If the string contains a lower number of characters than there are defined features for an API, all features that would be represented by characters that are not present in the string are not supported. |
| Uinteger | integer | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible. |
| UintegerRm | integer | This data type is defined in the same way as the "Uinteger" data type, but with the OpenAPI "nullable: true" property. |
| Uint32 | integer | Unsigned 32-bit integers, i.e. only value 0 and 32-bit integers above 0 are permissible. |
| Uint32Rm | integer | This data type is defined in the same way as the "UInt32" data type, but with the OpenAPI "nullable: true" property. |
| Uint64 | integer | Unsigned 64-bit integers, i.e. only value 0 and 64-bit integers above 0 are permissible. |
| Uint64Rm | integer | This data type is defined in the same way as the "Uint64" data type, but with the OpenAPI "nullable: true" property. |
| Uri | string | String providing an URI formatted according to IETF RFC 3986 [6]. |
| UriRm | string | This data type is defined in the same way as the "Uri" data type, but with the OpenAPI "nullable: true" property. |
| VarUeId | string | String represents the SUPI or GPSI.  Pattern: "^(imsi-[0-9]{5,15}|nai-.+|msisdn-[0-9]{5,15}|extid-[^@]+@[^@]+|.+)$". |
| VarUeIdRm | string | This data type is defined in the same way as the "VarUeId" data type, but with the OpenAPI "nullable: true" property. |
| TimeZone | string | String with format "<time-numoffset>" optionally appended by "<daylightSavingTime>", where:  - <time-numoffset> shall represent the time zone adjusted for daylight saving time and be encoded as time-numoffset as defined in clause 5.6 of IETF RFC 3339 [10];  - <daylightSavingTime> shall represent the adjustment that has been made and shall be encoded as "+1" or "+2" for a +1 or +2 hours adjustment.  Example: "-08:00+1" (for 8 hours behind UTC, +1 hour adjustment for Daylight Saving Time). |
| TimeZoneRm | string | This data type is defined in the same way as the "TimeZone" data type, but with the OpenAPI "nullable: true" property. |

Table 5.2.2-2: Reused OpenAPI data types

|  |  |
| --- | --- |
| Type Name | Description |
| boolean | As defined in OpenAPI Specification [3] |
| integer | As defined in OpenAPI Specification [3] |
| number | As defined in OpenAPI Specification [3] |
| string | As defined in OpenAPI Specification [3] |
| NOTE Data types defined in OpenAPI Specification [3] do not follow the UpperCamel convention for data types in 3GPP TS 29.501 [2] | |

Table 5.2.2-3: Meaning of a Hexadecimal Character in SupportedFeatures Type

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Character | Feature n+3 supported | Feature n+2 supported | Feature n+1 supported | Feature n supported |
| "0" | no | no | no | no |
| "1" | no | no | no | yes |
| "2" | no | no | yes | no |
| "3" | no | no | yes | yes |
| "4" | no | yes | no | no |
| "5" | no | yes | no | yes |
| "6" | no | yes | yes | no |
| "7" | no | yes | yes | yes |
| "8" | yes | no | no | no |
| "9" | yes | no | no | yes |
| "A" | yes | no | yes | no |
| "B" | yes | no | yes | yes |
| "C" | yes | yes | no | no |
| "D" | yes | yes | no | yes |
| "E" | yes | yes | yes | no |
| "F" | yes | yes | yes | yes |
| NOTE 1 "n" shall be i \* 4 + 1, where "i" is zero or a natural number, i.e permissible values of "n" are 1, 5, 9, …  NOTE 2 If a feature is not defined, it shall be indicated with value "no". | | | | |

For example, if only the first feature defined in the feature list is set to 1, the corresponding SupportedFeatures attribute would have a value of "1", or "001" (any amount of 0's to the left of the 1 would result into an equivalent feature list). If we have 32 features defined, and only the last feature in a feature list is set to 1, the corresponding SupportedFeatures attribute would have a value of "80000000".

### 5.2.3 Enumerations

#### 5.2.3.1 Enumeration: PatchOperation

Table 5.2.3.1-1: Enumeration PatchOperation

|  |  |
| --- | --- |
| Enumeration value | Description |
| "add" | Add operation as defined in IETF RFC 6902 [14]. |
| "copy" | Copy operation as defined in IETF RFC 6902 [14]. |
| "move" | Move operation as defined in IETF RFC 6902 [14]. |
| "remove" | Remove operation as defined in IETF RFC 6902 [14]. |
| "replace" | Replace operation as defined in IETF RFC 6902 [14]. |
| "test" | Test operation as defined in IETF RFC 6902 [14]. |

#### 5.2.3.2 Enumeration: UriScheme

Table 5.2.3.2-1: Enumeration UriScheme

|  |  |
| --- | --- |
| Enumeration value | Description |
| "http" | HTTP URI scheme |
| "https" | HTTPS URI scheme |

#### 5.2.3.3 Enumeration: ChangeType

Table 5.2.3.3-1: Enumeration ChangeType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "ADD" | This value indicates new attribute has been added to the resource |
| "MOVE" | This value indicates existing attribute has been moved to a different path in the resource. |
| "REMOVE" | This value indicates existing attribute has been deleted from the resource. |
| "REPLACE" | This value indicates existing attribute has been updated with new value. |

### 5.2.4 Structured Data Types

#### 5.2.4.1 Type: ProblemDetails

Table 5.2.4-1: Definition of type ProblemDetails

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| type | Uri | O | 0..1 | A URI reference according to IETF RFC 3986 [6] that identifies the problem type. |
| title | string | O | 0..1 | A short, human-readable summary of the problem type. It should not change from occurrence to occurrence of the problem. |
| status | integer | O | 0..1 | The HTTP status code for this occurrence of the problem. |
| detail | string | O | 0..1 | A human-readable explanation specific to this occurrence of the problem. |
| instance | Uri | O | 0..1 | A URI reference that identifies the specific occurrence of the problem. |
| cause | string | C | 0..1 | A machine-readable application error cause specific to this occurrence of the problem  This IE should be present and provide application-related error information, if available. |
| invalidParams | array(InvalidParam) | O | 1..N | Description of invalid parameters, for a request rejected due to invalid parameters. |
| supportedFeatures | SupportedFeatures | C | 0..1 | Features supported by the NF Service Producer.  This IE shall be present when rejecting a request due to an unsupported query parameter, if at least one feature is defined for the corresponding service in the version of the specification that the NF Service Producer implements (see clause 5.2.x of 3GPP TS 29.500 [25]).  When present, this IE shall indicate the features supported by the NF Service Producer; if the NF Service Producer supports no features, this IE shall be set to the character "0". |
| NOTE 1: See IETF RFC 7807 [9] for detailed information and guidance for each attribute, and 3GPP TS 29.501 [2] for guidelines on error handling support by 5GC SBI APIs.  NOTE 2: Additional attributes may be defined per API. | | | | |

#### 5.2.4.2 Type: Link

Table 5.2.4.2-1: Definition of type link

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| href | Uri | M | 1 | It contains the URI of the linked resource. |

#### 5.2.4.3 Type PatchItem

Table 5.2.4.3-1: Definition of type PatchItem

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| op | PatchOperation | M | 1 | This IE indicates the patch operation as defined in IETF RFC 6902 [14] to be performed on resource. |  |
| path | string | M | 1 | This IE contains a JSON pointer value (as defined in IETF RFC 6901 [12]) that references a location of a resource on which the patch operation shall be performed. |  |
| from | string | C | 0..1 | This IE indicates the path of the source JSON element (according to JSON Pointer syntax) being moved or copied to the location indicated by the "path" attribute.  It shall be present if the patch operation is "move" or "copy". |  |
| value | Any type | C | 0..1 | This IE indicates a new value for the resource specified in the path attribute.  It shall be present if the patch operation is "add", "replace" or "test".  The data type of this attribute shall be the same as the type of the resource on which the patch operation shall be performed. The null value shall be allowed. |  |

#### 5.2.4.4 Type: LinksValueSchema

Table 5.2.4.4-1: Definition of type LinksValueSchema as a list of mutually exclusive alternatives

|  |  |  |
| --- | --- | --- |
| Data type | Cardinality | Description |
| array(Link) | 1..N | Array of links |
| Link | 1 | link |

#### 5.2.4.5 Type: SelfLink

Table 5.2.4.5-1: Definition of type SelfLink

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| self | Link | M | 1 | It contains the URI of the linked resource. |

#### 5.2.4.6 Type: InvalidParam

Table 5.2.4.6-1: Definition of type InvalidParam

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| param | string | M | 1 | Attribute's name encoded as a JSON Pointer. |
| reason | string | O | 0..1 | A human-readable reason, e.g. "must be a positive integer". |

#### 5.2.4.7 Type: LinkRm

This data type is defined in the same way as the "Link" data type, but with the OpenAPI "nullable: true" property.

#### 5.2.4.8 Type ChangeItem

Table 5.2.4.8-1: Definition of type ChangeItem

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| op | ChangeType | M | 1 | This IE indicates the change type which happens to the resource. |  |
| path | string | M | 1 | This IE contains a JSON pointer value (as defined in IETF RFC 6901 [12]) that references a target location within the resource on which the change has been applied.  (See Note) |  |
| from | string | C | 0..1 | This IE indicates the path of the source JSON element (according to JSON Pointer syntax) being moved or copied to the location indicated by the "path" attribute.  It shall be present if the "op" attribute is of value "MOVE". |  |
| origValue | Any type | O | 0..1 | This IE indicates the original value at the target location within the resource specified in the path attribute. This attribute only applies when the "op" attribute is of value "REMOVE", "REPLACE" or "MOVE"  Based on the use case, this attribute may be included. |  |
| newValue | Any type | C | 0..1 | This IE indicates a new value at the target location within the resource specified in the path attribute.  It shall be present if the "op" attribute is of value "ADD", "REPLACE".  The data type of this attribute shall be the same as the type of the resource on which the change has happened. The null value shall be allowed. |  |
| NOTE: As described in IETF RFC 6901 [12], the value "" (empty JSON string) is the JSON Pointer expression to represent "the whole JSON document"; therefore, when the attribute "path" takes value "" and attribute "op" takes values "ADD" or "REMOVE", this shall be interpreted as the creation or deletion respectively of the resource to which this "ChangeItem" refers to. | | | | | |

#### 5.2.4.9 Type NotifyItem

Table 5.2.4.9-1: Definition of type NotifyItem

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| resourceId | Uri | M | 1 | This IE contains the URI of the resource which has been changed. |  |
| changes | array(ChangeItem) | M | 1..N | This IE contains the changes which have been applied on the resource identified by the resourceId attribute. |  |

#### 5.2.4.10 Type: ComplexQuery

Table 5.2.4.10-1: Definition of type ComplexQuery as a list of mutually exclusive alternatives

|  |  |  |
| --- | --- | --- |
| Data type | Cardinality | Description |
| Cnf | 1 | A conjunctive normal form |
| Dnf | 1 | A disjunctive normal form |

The ComplexQuery data type is either a conjunctive normal form or a disjunctive normal form. The attribute names "cnfUnits" and "dnfUnits" (see clause 5.2.4.11 and clause 5.2.4.12) serve as discriminator.

#### 5.2.4.11 Type: Cnf

Table 5.2.4.11-1: Definition of type Cnf

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| cnfUnits | array(CnfUnit) | M | 1..N | During the processing of cnfUnits attribute, all the members in the array shall be interpreted as logically concatenated with logical "AND". |  |

#### 5.2.4.12 Type: Dnf

Table 5.2.4.12-1: Definition of type Dnf

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnfUnits | array(DnfUnit) | M | 1..N | During the processing of dnfUnits attribute, all the members in the array shall be interpreted as logically concatenated with logical "OR". |  |

#### 5.2.4.13 Type: CnfUnit

Table 5.2.4.13-1: Definition of type CnfUnit

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| cnfUnit | array(Atom) | M | 1..N | During the processing of cnfUnit attribute, all the members in the array shall be interpreted as logically concatenated with logical "OR". |  |

#### 5.2.4.14 Type: DnfUnit

Table 5.2.4.14-1: Definition of type DnfUnit

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnfUnit | array(Atom) | M | 1..N | During the processing of dnfUnit attribute, all the members in the array shall be interpreted as logically concatenated with logical "AND". |  |

#### 5.2.4.15 Type: Atom

Table 5.2.4.15-1: Definition of type Atom

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| attr | string | M | 1 | This attribute contains the name of a defined query parameter. |  |
| value | any type | M | 1 | This attribute contains the value of the query parameter as indicated by attr attribute. |  |
| negative | boolean | O | 0..1 | This attribute indicates whether the negative condition applies for the query condition. |  |

#### 5.2.4.16 Type: NFDiscFactors

Table 5.2.4.16-1: Definition of type NFDiscFactors

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| targetNfType | NFType | O | 0..1 | See "target-nf-type" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| requesterNfType | NFType | O | 0..1 | See "requester-nf-type" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| serviceNames | array(ServiceName) | O | 1..N | See "service-names" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| requesterNfInstanceFqdn | Fqdn | O | 0..1 | See "requester-nf-instance-fqdn" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| targetPlmnList | array(PlmnId) | O | 1..N | See "target-plmn-list" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| requesterPlmnList | array(PlmnId) | O | 1..N | See "requester-plmn-list" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| targetNfInstanceId | NfInstanceId | O | 0..1 | See "target-nf-instance-id" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| targetNfFqdn | Fqdn | O | 0..1 | See "target-nf-fqdn" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| hnrfUri | Uri | O | 0..1 | See "hnrf-uri" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| snssais | array(Snssai) | O | 1..N | See "snssais" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| plmnSpecificSnssaiList | array(PlmnSnssai) | O | 1..N | See "plmn-specific-snssai-list" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| nsiList | array(string) | O | 1..N | See "nsi-list" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| dnn | Dnn | O | 0..1 | See "dnn" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| tai | Tai | O | 0..1 | See "tai" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| amfRegionId | AmfRegionId | O | 0..1 | See "amf-region-id" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| amfSetId | AmfSetId | O | 0..1 | See "amf-set-id" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| guami | Guami | O | 0..1 | See "guami" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| supi | Supi | O | 0..1 | See "supi" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| ueIpv4Address | Ipv4Addr | O | 0..1 | See " ue-ipv4-address " in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| ipDomain | string | O | 0..1 | See "ip-domain" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| ueIpv6Prefix | Ipv6Prefix | O | 0..1 | See "ue-ipv6-prefix" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| pgwInd | boolean | O | 0..1 | See "pgw-ind" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| pgw | Fqdn | O | 0..1 | See "pgw" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| gpsi | Gpsi | O | 0..1 | See "gpsi" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| externalGroupIdentity | GroupId | O | 0..1 | See "external-group-identity" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| dataSet | DataSetId | O | 0..1 | See "data-set" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| routingIndicator | string | O | 0..1 | See "routing-indicator" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| groupIdList | array(NfGroupId) | O | 1..N | See "group-id-list" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| dnaiList | array(Dnai) | O | 1..N | See "dnai-list" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| upfIwkEpsInd | boolean | O | 0..1 | See "upf-iwk-eps-ind" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| chfSupportedPlmn | PlmnId | O | 0..1 | See "chf-supported-plmn" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| preferredLocality | string | O | 0..1 | See "preferred-locality" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| accessType | AccessType | O | 0..1 | See "access-type" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| requiredFeatures | array(SupportedFeatures) | O | 1..N | See "required-features" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| complexQuery | ComplexQuery | O | 0..1 | See "complex-query" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |
| pduSessionTypes | array(PduSessionType) | O | 1..N | See "pdu-session-types" in 3GPP TS 29.510 [29], Table 6.2.3.2.3.1-1. |

Editor's Note: This table needs further review.

## 5.3 Data Types related to Subscription, Identification and Numbering

### 5.3.1 Introduction

This clause defines common data types related to subscription, identification and numbering information.

### 5.3.2 Simple Data Types

This clause specifies common simple data types.

Table 5.3.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
| Dnn | string | String representing a Data Network as defined in clause 9A of 3GPP TS 23.003 [7]. It shall be formatted as string in which the labels are separated by dots (e.g. "Label1.Label2.Label3"). |
| DnnRm | string | This data type is defined in the same way as the "Dnn" data type, but with the OpenAPI "nullable: true" property. |
| Gpsi | string | String identifying a Gpsi shall contain either an External Id or an MSISDN. It shall be formatted as follows:  -External Identifier: "extid-<extid>, where <extid> shall be formatted according to clause 19.7.2 of 3GPP TS 23.003 [7] that describes an External Identifier.  -MSISDN: "msisdn-<msisdn>, where <msisdn> shall be formatted according to clause 3.3 of 3GPP TS 23.003 [7] that describes an MSISDN.  Pattern: '^(msisdn-[0-9]{5,15}|extid-.+@.+|.+)$' |
| GpsiRm | string | This data type is defined in the same way as the "Gpsi" data type, but with the OpenAPI "nullable: true" property. |
| GroupId | string | String identifying a group of devices network internal globally unique ID which identifies a set of IMSIs, as specified in clause 19.9 of 3GPP TS 23.003 [7].  Pattern: '^[A-Fa-f0-9]{8}-[0-9]{3}-[0-9]{2,3}-([A-Fa-f0-9][A-Fa-f0-9]){1,10}$'. |
| GroupIdRm | string | This data type is defined in the same way as the "GroupId" data type, but with the OpenAPI "nullable: true" property. |
| Pei | string | String representing a Permanent Equipment Identifier, if it contains an IMEI or IMEISV it is defined as specified in clause 6.2 of 3GPP TS 23.003 [7].  Pattern: '^(imei-[0-9]{15}|imeisv-[0-9]{16}|.+)$'. See NOTE. |
| PeiRm | string | This data type is defined in the same way as the "Pei" data type, but with the OpenAPI "nullable: true" property. |
| Supi | string | String identifying a Supi shall contain either an IMSI or an NAI. It shall be formatted as follows for:  - IMSI "imsi-<imsi>, <imsi> shall be formatted according to clause 2.2 of 3GPP TS 23.003 [7] that describes an IMSI.  - NAI "nai-<nai>, <nai> shall be formatted according to clause 28.6.2 of 3GPP TS 23.003 [7] that describes an NAI.  To enable that the value is used as part of an URI, the string shall only contain characters allowed according to the "lower-with-hyphen" naming convention defined in 3GPP TS 29.501 [2].  Pattern: '^(imsi-[0-9]{5,15}|nai-.+|.+)$'. See NOTE. |
| SupiRm | string | This data type is defined in the same way as the "Supi" data type, but with the OpenAPI "nullable: true" property. |
| NfInstanceId | string | String uniquely identifying a NF instance. The format of the NF Instance ID shall be a Universally Unique Identifier (UUID) version 4, as described in IETF RFC 4122 [15]. |
| AmfId | string | String identifying the AMF ID composed of AMF Region ID (8 bits), AMF Set ID (10 bits) and AMF Pointer (6 bits) as specified in clause 2.10.1 of 3GPP TS 23.003 [7].  It is encoded as a string of 6 hexadecimal characters (i.e., 24 bits).  Pattern: '^[A-Fa-f0-9]{6}$' |
| AmfRegionId | string | String identifying the AMF Region ID (8 bits), as specified in clause 2.10.1 of 3GPP TS 23.003 [7].  It is encoded as a string of 2 hexadecimal characters (i.e. 8 bits).  Pattern: '^[A-Fa-f0-9]{2}$' |
| AmfSetId | string | String identifying the AMF Set ID (10 bits) as specified in clause 2.10.1 of 3GPP TS 23.003 [7].  It is encoded as a string of 3 hexadecimal characters where the first character is limited to values 0 to 3 (i.e. 10 bits).  Pattern: '^[0-3][A-Fa-f0-9]{2}$' |
| RfspIndex | integer | Unsigned integer representing the "Subscriber Profile ID for RAT/Frequency Priority" as specified in 3GPP TS 36.413 [16].  Minimum = 1. Maximum = 256. |
| RfspIndexRm | integer | This data type is defined in the same way as the "RfspIndex" data type, but with the OpenAPI "nullable: true" property. |
| NfGroupId | string | Identifier of a group of NFs |
| MtcProviderInformation | string | String uniquely identifying MTC provider information. |
| NOTE: The encoding of 3GPP defined identifiers (e.g. IMSI, NAI) shall be prefixed with its corresponding prefix (e.g. 'imsi-','nai-'). | | |

### 5.3.3 Enumerations

For Data Types related to Subscription, Identification and Numbering, no Enumerations data types are defined in this version of the specification.

### 5.3.4 Structured Data Types

#### 5.3.4.1 Type: Guami

Table 5.3.4.1-1: Definition of type Guami

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| plmnId | PlmnId | M | 1 | PLMN Identity |
| amfId | AmfId | M | 1 | AMF Identity |

#### 5.3.4.2 Type: NetworkId

Table 5.3.4.2-1: Definition of type NetworkId

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| mcc | Mcc | C | 0..1 | Mobile Country Code |
| mnc | Mnc | C | 0..1 | Mobile Network Code |
| NOTE: At least one MNC or MCC shall be included. | | | | |

#### 5.3.4.3 Type: GuamiRm

This data type is defined in the same way as the "Guami" data type, but with the OpenAPI "nullable: true" property.

## 5.4 Data Types related to 5G Network

### 5.4.1 Introduction

This clause defines common data types related to 5G Network (other than related to 5G QoS).

### 5.4.2 Simple Data Types

This clause specifies common simple data types.

Table 5.4.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
| ApplicationId | string | String providing an application identifier. |
| ApplicationIdRm | string | This data type is defined in the same way as the "ApplicationId" data type, but with the OpenAPI "nullable: true" property. |
| PduSessionId | integer | Unsigned integer identifying a PDU session, within the range 0 to 255, as specified in clause 11.2.3.1b, bits 1 to 8, of 3GPP TS 24.007 [13]. |
| Mcc | string | Mobile Country Code part of the PLMN, comprising 3 digits, as defined in clause 9.3.3.5 of 3GPP TS 38.413 [11].  Pattern: '^[0-9]{3}$' |
| MccRm | string | This data type is defined in the same way as the "Mcc" data type, but with the OpenAPI "nullable: true" property. |
| Mnc | string | Mobile Network Code part of the PLMN, comprising 2 or 3 digits, as defined in clause 9.3.3.5 of 3GPP TS 38.413 [11].  Pattern: '^[0-9]{2,3}$' |
| MncRm | string | This data type is defined in the same way as the "Mnc" data type, but with the OpenAPI "nullable: true" property. |
| Tac | string | 2 or 3-octet string identifying a tracking area code as specified in clause 9.3.3.10 of 3GPP TS 38.413 [11], in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the TAC shall appear first in the string, and the character representing the 4 least significant bit of the TAC shall appear last in the string.  Examples:  A legacy TAC 0x4305 shall be encoded as "4305".  An extended TAC 0x63F84B shall be encoded as "63F84B" |
| TacRm | string | This data type is defined in the same way as the "Tac" data type, but with the OpenAPI "nullable: true" property. |
| EutraCellId | string | 28-bit string identifying an E-UTRA Cell Id as specified in clause 9.3.1.9 of 3GPP TS 38.413 [11], in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the Cell Id shall appear first in the string, and the character representing the 4 least significant bit of the Cell Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{7}$'  Example:  An E-UTRA Cell Id 0x5BD6007 shall be encoded as "5BD6007". |
| EutraCellIdRm | string | This data type is defined in the same way as the "EutraCellId" data type, but with the OpenAPI "nullable: true" property. |
| NrCellId | string | 36-bit string identifying an NR Cell Id as specified in clause 9.3.1.7 of 3GPP TS 38.413 [11], in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the Cell Id shall appear first in the string, and the character representing the 4 least significant bit of the Cell Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{9}$'  Example:  An NR Cell Id 0x225BD6007 shall be encoded as "225BD6007". |
| NrCellIdRm | string | This data type is defined in the same way as the "NrCellId" data type, but with the OpenAPI "nullable: true" property. |
| Dnai | string | DNAI (Data network access identifier), see clause 5.6.7 of 3GPP TS 23.501 [8]. |
| DnaiRm | string | This data type is defined in the same way as the "Dnai" data type, but with the OpenAPI "nullable: true" property. |
| 5GMmCause | Uinteger | This represents the 5GMM cause code values as specified in 3GPP TS 24.501 [20]. |
| AreaCodeRm | string | This data type is defined in the same way as the "AreaCode" data type, but with the OpenAPI "nullable: true" property. |
| AmfName | string | FQDN (Fully Qualified Domain Name) of the AMF as defined in clause 28.3.2.5 of 3GPP TS 23.003 [7]. |
| AreaCode | string | Values are operator specific. |
| N3IwfId | string | This represents the identifier of the N3IWF ID as specified in clause 9.3.1.57 of 3GPP TS 38.413 [11].  Pattern: '^[A-Fa-f0-9]+$' |
| NgeNbId | string | This represents the identifier of the ng-eNB ID as specified in clause 9.3.1.8 of 3GPP TS 38.413 [11]..  The string shall be formatted with following pattern:  Pattern: '^('MacroNGeNB-[A-Fa-f0-9]{5}|  LMacroNGeNB-[A-Fa-f0-9]{6}|  SMacroNGeNB-[A-Fa-f0-9]{5})$'  The value of the ng-eNB ID shall be encoded in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The padding 0 shall be added to make multiple nibbles, so the most significant character representing the padding 0 if required together with the 4 most significant bits of the ng-eNB ID shall appear first in the string, and the character representing the 4 least significant bit of the ng-eNB ID (to form a nibble) shall appear last in the string.  Examples:  " SMacroNGeNB-34B89" indicates a Short Macro NG-eNB ID with value 0x34B89. |

### 5.4.3 Enumerations

#### 5.4.3.1 Enumeration: AccessType

Table 5.4.3.1-1: Enumeration AccessType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "3GPP\_ACCESS" | 3GPP access |
| "NON\_3GPP\_ACCESS" | Non-3GPP access |

#### 5.4.3.2 Enumeration: RatType

Table 5.4.3.2-1: Enumeration RatType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "NR" | New Radio |
| "EUTRA" | (WB) Evolved Universal Terrestrial Radio Access |
| "WLAN" | Wireless LAN |
| "VIRTUAL" | Virtual (see NOTE) |
| "NBIOT" | NB IoT |
| NOTE: Virtual shall be used if the N3IWF does not know the access technology used for an untrusted non-3GPP access. | |

#### 5.4.3.3 Enumeration: PduSessionType

The enumeration PduSessionType indicates the type of a PDU session. It shall comply with the provisions defined in table 5.4.3.3-1.

Table 5.4.3.3-1: Enumeration PduSessionType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "IPV4" | IPv4 |
| "IPV6" | IPv6 |
| "IPV4V6" | IPv4v6 (see clause 5.8.2.2.1 of 3GPP TS 23.501 [8]) |
| "UNSTRUCTURED" | Unstructured |
| "ETHERNET" | Ethernet |

#### 5.4.3.4 Enumeration: UpIntegrity

The enumeration UpIntegrity indicates whether UP integrity protection is required, preferred or not needed for all the traffic on the PDU Session. It shall comply with the provisions defined in table 5.4.3.4-1.

Table 5.4.3.4-1: Enumeration UpIntegrity

|  |  |
| --- | --- |
| Enumeration value | Description |
| "REQUIRED" | UP integrity protection shall apply for all the traffic on the PDU Session. |
| "PREFERRED" | UP integrity protection should apply for all the traffic on the PDU Session. |
| "NOT\_NEEDED" | UP integrity protection shall not apply on the PDU Session. |

#### 5.4.3.5 Enumeration: UpConfidentiality

The enumeration UpConfidentiality indicates whether UP confidentiality protection is required, preferred or not needed for all the traffic on the PDU Session. It shall comply with the provisions defined in table 5.4.3.5-1.

Table 5.4.3.5-1: Enumeration UpConfidentiality

|  |  |
| --- | --- |
| Enumeration value | Description |
| "REQUIRED" | UP confidentiality protection shall apply for all the traffic on the PDU Session. |
| "PREFERRED" | UP confidentiality protection should apply for all the traffic on the PDU Session. |
| "NOT\_NEEDED" | UP confidentiality protection shall not apply on the PDU Session. |

#### 5.4.3.6 Enumeration: SscMode

The enumeration SscMode represents the service and session continuity mode.

Table 5.4.3.6-1: Enumeration SscMode

|  |  |
| --- | --- |
| Enumeration value | Description |
| "SSC\_MODE\_1" | see 3GPP TS 23.501 [2] |
| "SSC\_MODE\_2" | see 3GPP TS 23.501 [2] |
| "SSC\_MODE\_3" | see 3GPP TS 23.501 [2] |

#### 5.4.3.7 Enumeration: DnaiChangeType

The enumeration DnaiChangeType represents the type of a DNAI change. A NF service consumer may subscribe to "EARLY", "LATE" or "EARLY\_LATE" types of DNAI change. The types of observed DNAI change the SMF may notify are "EARLY" or "LATE". The DnaiChangeType data type shall comply with the provisions defined in table 5.4.3.7-1.

Table 5.4.3.7-1: Enumeration DnaiChangeType

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| EARLY | Early notification of UP path reconfiguration. |  |
| EARLY\_LATE | Early and late notification of UP path reconfiguration. This value shall only be present in the subscription to the DNAI change event. |  |
| LATE | Late notification of UP path reconfiguration. |  |

#### 5.4.3.8 Enumeration: RestrictionType

Table 5.4.3.8-1: Enumeration RestrictionType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "ALLOWED\_AREAS" | This value indicates that areas are allowed. |
| "NOT\_ALLOWED\_AREAS" | This value indicates that areas are not allowed. |

#### 5.4.3.9 Enumeration: CoreNetworkType

Table 5.4.3.9-1: Enumeration CoreNetworkType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "5GC" | 5G Core |
| "EPC" | Evolved Packet Core |

#### 5.4.3.10 Enumeration: AccessTypeRm

This enumeration is defined in the same way as the "AccessType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.11 Enumeration: RatTypeRm

This enumeration is defined in the same way as the "RatType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.12 Enumeration: PduSessionTypeRm

This enumeration is defined in the same way as the "PduSessionType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.13 Enumeration: UpIntegrityRm

This enumeration is defined in the same way as the "UpIntegrity" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.14 Enumeration: UpConfidentialityRm

This enumeration is defined in the same way as the "UpConfidentiality" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.15 Enumeration: SscModeRm

This data type is defined in the same way as the "SscMode" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.17 Enumeration: DnaiChangeTypeRm

This data type is defined in the same way as the "DnaiChangeType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.18 Enumeration: RestrictionTypeRm

This data type is defined in the same way as the "RestrictionType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.19 Enumeration: CoreNetworkType

This data type is defined in the same way as the "CoreNetworkType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.4.3.20 Enumeration: PresenceState

Table 5.4.3.20-1: Enumeration PresenceState

|  |  |
| --- | --- |
| Enumeration value | Description |
| "IN\_AREA" | Indicates that the UE is inside or enters the presence reporting area. |
| "OUT\_OF\_AREA" | Indicates that the UE is outside or leaves the presence reporting area. |
| "UNKNOWN" | Indicates it is unknown whether the UE is in the presence reporting area or not. |
| "INACTIVE" | Indicates that the presence reporting area is inactive in the serving node. |

### 5.4.4 Structured Data Types

#### 5.4.4.1 Type: SubscribedDefaultQos

Table 5.4.4.1-1: Definition of type SubscribedDefaultQos

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| 5qi | 5Qi | M | 1 | Default 5G QoS identifier see 3GPP TS 23.501 [8] clause 5.7.2.7. |
| arp | Arp | M | 1 | Default Allocation and Retention Priority see 3GPP TS 23.501 [8] clause 5.7.2.7. |
| priorityLevel | 5QiPriorityLevel | O | 0..1 | Defines the 5QI Priority Level.  When present, it contains the 5QI Priority Level value that overrides the standardized or pre-configured value as described in 3GPP TS 23.501 [8]. |

#### 5.4.4.2 Type: Snssai

Table 5.4.4.2-1: Definition of type Snssai

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| sst | Uinteger | M | 1 | Unsigned integer, within the range 0 to 255, representing the Slice/Service Type. It indicates the expected Network Slice behaviour in terms of features and services.  Values 0 to 127 correspond to the standardized SST range. Values 128 to 255 correspond to the Operator-specific range. See clause 28.4.2 of 3GPP TS 23.003 [7].  Standardized values are defined in clause 5.15.2.2 of 3GPP TS 23.501 [8]. |
| sd | string | O | 0..1 | 3-octet string, representing the Slice Differentiator, in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the SD shall appear first in the string, and the character representing the 4 least significant bit of the SD shall appear last in the string.  This is an optional parameter that complements the Slice/Service type(s) to allow to differentiate amongst multiple Network Slices of the same Slice/Service type.  Pattern: '^[A-Fa-f0-9]{6}$' |

When Snssai needs to be converted to string (e.g. when used in maps as key), the string shall be composed of one to three digits "sst" optionally followed by "-" and 6 hexadecimal digits "sd", and shall match the following pattern:

^([0-9]|[1-9][0-9]|1[0-9][0-9]|2([0-4][0-9]|5[0-5]))(-[A-Fa-f0-9]{6})?$

Example 1: "255-19CDE0"

Example 2: "29"

#### 5.4.4.3 Type: PlmnId

Table 5.4.4.3-1: Definition of type PlmnId

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| mcc | Mcc | M | 1 | Mobile Country Code |
| mnc | Mnc | M | 1 | Mobile Network Code |

#### 5.4.4.4 Type: Tai

Table 5.4.4.4-1: Definition of type Tai

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| plmnId | PlmnId | M | 1 | PLMN Identity |
| tac | Tac | M | 1 | Tracking Area Code |

#### 5.4.4.5 Type: Ecgi

Table 5.4.4.5-1: Definition of type Ecgi

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| plmnId | PlmnId | M | 1 | PLMN Identity |
| eutraCellId | EutraCellId | M | 1 | E-UTRA Cell Identity |

#### 5.4.4.6 Type: Ncgi

Table 5.4.4.6-1: Definition of type Ncgi

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| plmnId | PlmnId | M | 1 | PLMN Identity |
| nrCellId | NrCellId | M | 1 | NR Cell Identity |

#### 5.4.4.7 Type: UserLocation

Table 5.4.4.7-1: Definition of type UserLocation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| eutraLocation | EutraLocation | C | 0..1 | E-UTRA user location (see NOTE). |
| nrLocation | NrLocation | C | 0..1 | NR user location (see NOTE). |
| n3gaLocation | N3gaLocation | C | 0..1 | Non-3GPP access user location (see NOTE). |
| NOTE: At least one of eutraLocation, nrLocation and n3gaLocation shall be present. Several of them may be present. | | | | |

#### 5.4.4.8 Type: EutraLocation

Table 5.4.4.8-1: Definition of type EutraLocation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| tai | Tai | M | 1 | Tracking Area Identity |
| ecgi | Ecgi | M | 1 | E-UTRA Cell Identity |
| ageOfLocationInformation | integer | O | 0 1 | The value represents the elapsed time in minutes since the last network contact of the mobile station.  Value "0" indicates that the location information was obtained after a successful paging procedure for Active Location Retrieval when the UE is in idle mode or after a successful NG-RAN location reporting procedure with the eNB when the UE is in connected mode.  Any other value than "0" indicates that the location information is the last known one.  See 3GPP TS 29.002 [21] clause 17.7.8. |
| ueLocationTimestamp | DateTime | O | 0..1 | The value represents the UTC time when the UeLocation information was acquired. |
| geographicalInformation | string | O | 0..1 | Refer to geographical Information.  See 3GPP TS 23.032 [23] clause 7.3.2. Only the description of an ellipsoid point with uncertainty circle is allowed to be used.  Allowed characters are 0-9 and A-F; |
| geodeticInformation | string | O | 0..1 | Refers to Calling Geodetic Location.  See ITU-T Recommendation Q.763 (1999) [24] clause 3.88.2. Only the description of an ellipsoid point with uncertainty circle is allowed to be used.  Allowed characters are 0-9 and A-F. |
| globalNgenbId | GlobalRanNodeId | O | 0..1 | It indicates the global identity of the ng-eNodeB in which the UE is currently located.  See 3GPP TS 38.413 [11] clause 9.3.1.8. |

#### 5.4.4.9 Type: NrLocation

Table 5.4.4.9-1: Definition of type NrLocation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| tai | Tai | M | 1 | Tracking Area Identity |
| ncgi | Ncgi | M | 1 | NR Cell Identity |
| ageOfLocationInformation | integer | O | 0 1 | The value represents the elapsed time in minutes since the last network contact of the mobile station.  Value "0" indicates that the location information was obtained after a successful paging procedure for Active Location Retrieval when the UE is in idle mode or after a successful NG-RAN location reporting procedure with the gNB when the UE is in connected mode.  Any other value than "0" indicates that the location information is the last known one.  See 3GPP TS 29.002 [21] clause 17.7.8. |
| ueLocationTimestamp | DateTime | O | 0..1 | The value represents the UTC time when the UeLocation information was acquired. |
| geographicalInformation | string | O | 0..1 | Refer to geographical Information.  See 3GPP TS 23.032 [23] clause 7.3.2. Only the description of an ellipsoid point with uncertainty circle is allowed to be used.  Allowed characters are 0-9 and A-F; |
| geodeticInformation | string | O | 0..1 | Refers to Calling Geodetic Location.  See ITU-T Recommendation Q.763 (1999) [24] clause 3.88.2. Only the description of an ellipsoid point with uncertainty circle is allowed to be used.  Allowed characters are 0-9 and A-F. |
| globalGnbId | GlobalRanNodeId | O | 0..1 | It indicates the global identity of the gNodeB in which the UE is currently located.  See 3GPP TS 38.413 [11] clause 9.3.1.6. |

#### 5.4.4.10 Type: N3gaLocation

Table 5.4.4.10-1: Definition of type N3gaLocation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n3gppTai | Tai | C | 0..1 | The unique non 3GPP TAI used in the PLMN. It shall be present over the 3GPP PLMN internal interfaces, but shall not be present over the N5 interface. |
| n3IwfId | string | C | 0..1 | This IE shall contain the N3IWF identifier received over NGAP and shall be encoded as a string of hexadecimal characters.  Pattern: '^[A-Fa-f0-9]+$'  It shall be present over the 3GPP PLMN internal interfaces, but shall not be present over the N5 interface. |
| ueIpv4Addr | Ipv4Addr | C | 0..1 | UE local IPv4 address (used to reach the N3IWF).  The ueIPv4Addr or the ueIPv6Addr shall be present. |
| ueIpv6Addr | Ipv6Addr | C | 0..1 | UE local IPv6 address (used to reach the N3IWF).  The ueIPv4Addr or the ueIPv6Addr shall be present. |
| portNumber | Uinteger | C | 0..1 | UDP or TCP source port number. It shall be present if NAT is detected. |

#### 5.4.4.11 Type: UpSecurity

Table 5.4.4.11-1: Definition of type UpSecurity

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| upIntegr | UpIntegrity | M | 1 | This IE shall indicate whether UP integrity protection is required, preferred or not needed for all the traffic on the PDU Session. |
| upConfid | UpConfidentiality | M | 1 | This IE shall indicate whether UP confidentiality protection is required, preferred or not needed for all the traffic on the PDU Session. |

#### 5.4.4.12 Type: NgApCause

Table 5.4.4.12-1: Definition of type NgApCause

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| group | Uinteger | M | 1 | This IE shall indicate the group of the NGAP cause. The value of this IE shall equal to the ASN.1 value of the specified NGAP cause group.  NGAP supports following cause groups defined as separate enumerations, as specified in clause 9.4.5 of 3GPP TS 38.413 [11], with following values:  0 – radioNetwork  1 – transport  2 – nas  3 – protocol  4 – misc |
| value | Uinteger | M | 1 | This IE shall carry the NG AP cause value in specific cause group identified by the "group" attribute, as specified in clause 9.4.5 of 3GPP TS 38.413 [11]. |

#### 5.4.4.13 Type: BackupAmfInfo

Table 5.4.4.13-1: Definition of type BackupAmfInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| backupAmf | AmfName | M | 1 | This IE shall contain the AMF name of the backup AMF related to the specific GUAMI(s) (see clause 5.21.2.3 of 3GPP TS 23.501 [2]). If no GUAMI is included in BackupAmfinfo, the AMF name of the backup AMF is related to all the GUAMI(s) supported by the AMF. |
| guamiList | array(Guami) | C | 1..N | If present, this IE shall contain the GUAMI(s). |

#### 5.4.4.14 Type: RefToBinaryData

Table 5.4.4.14-1: Definition of type RefToBinaryData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| contentId | string | M | 1 | This IE shall contain the value of the Content-ID header of the referenced binary body part. |

#### 5.4.4.15 Type RouteToLocation

Table 5.4.4.15-1: Definition of type RouteToLocation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| dnai | Dnai | M | 1 | Identifies the location of the application. |
| routeInfo | RouteInformation | C | 0..1 | Includes the traffic routing information. |
| routeProfId | string | C | 0..1 | Identifies the routing profile Id. |
| NOTE: Either the "routeInfo" attribute or the "routeProfId" attribute shall be included in the "RouteToLocation" data type. | | | | |

#### 5.4.4.16 Type RouteInformation

Table 5.4.4.16-1: Definition of type RouteInformation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ipv4Addr | Ipv4Addr | C | 0..1 | Ipv4address of the tunnel end point in the data network. |
| ipv6Addr | Ipv6Addr | C | 0..1 | Ipv6 address of the tunnel end point in the data network. |
| portNumber | Uinteger | M | 1 | UDP port number of the tunnel end point in the data network. |
| NOTE: At least one of the "ipv4Addr" attribute and the "ipv6Addr" attribute shall be included in the "RouteInformation" data type. | | | | |

#### 5.4.4.17 Type: Area

Table 5.4.4.17-1: Definition of type Area

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| tacs | array(Tac) | C | 1..N | List of TACs; shall be present if and only if areaCode is absent. |
| areaCode | AreaCode | C | 0..1 | Area Code; shall be present if and only if tacs is absent. |

#### 5.4.4.18 Type: ServiceAreaRestriction

Table 5.4.4.18-1: Definition of type ServiceAreaRestriction

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| restrictionType | RestrictionType | C | 0..1 | string "ALLOWED\_AREAS" or "NOT\_ALLOWED\_AREAS"  shall be present if and only if the areas attribute is present |
| areas | array(Area) | O | 0..N  (NOTE) | A list of Areas.  These areas are:  - allowed areas if RestrictionType is "ALLOWED\_AREAS"  - not allowed areas if RestrictionType is "NOT\_ALLOWED\_AREAS" |
| maxNumOfTAs | Uinteger | C | 0..1 | Maximum number of allowed tracking areas for use when restrictionType indicates "ALLOWED\_AREAS".  This attribute shall be absent when attribute "restrictionType" takes the value "NOT\_ALLOWED\_AREAS". |
| maxNumOfTAsForNotAllowedAreas | Uinteger | C | 0..1 | Maximum number of allowed tracking areas for use when restrictionType indicates "NOT\_ALLOWED\_AREAS".  This attribute shall be absent when attribute "restrictionType" takes the value "ALLOWED\_AREAS". |
| NOTE: The empty array is used when service is allowed/restricted nowhere. | | | | |

#### 5.4.4.19 Type: PlmnIdRm

This data type is defined in the same way as the "PlmnId" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.20 Type: TaiRm

This data type is defined in the same way as the "Tai" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.21 Type: EcgiRm

This data type is defined in the same way as the "Ecgi" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.22 Type: NcgiRm

This data type is defined in the same way as the "Ncgi" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.23 Type: EutraLocationRm

This data type is defined in the same way as the "EutraLocation" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.24 Type: NrLocationRm

This data type is defined in the same way as the "NrLocation" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.25 Type: UpSecurityRm

This data type is defined in the same way as the "UpSecurity" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.26 Type: RefToBinaryDataRm

This data type is defined in the same way as the " RefToBinaryData " data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.27 Type: PresenceInfo

Table 5.4.4.27-1: Definition of type PresenceInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| praId | String | C | 0..1 | Represents an identifier to the specified area. This IE shall be present if the Area of Interest subscribed or reported is a Presence Reporting Area. |
| presenceState | PresenceState | C | 0..1 | Indicates whether the UE is inside or outside of the area of interest (e.g presence reporting area or the LADN area), or if the presence reporting area is inactive in the serving node. |
| trackingAreaList | array(Tai) | C | 1..N | Represents the list of tracking areas that constitutes the area. This IE shall be present if the subscription or the event report is for tracking UE presence in the tracking areas. For non 3GPP access the TAI shall be the N3GPP TAI. |
| ecgiList | array(Ecgi) | C | 1..N | Represents the list of EUTRAN cell Ids that constitutes the area. This IE shall be present if the Area of Interest subscribed is a list of EUTRAN cell Ids. |
| ncgiList | array(Ncgi) | C | 1..N | Represents the list of NR cell Ids that constitutes the area. This IE shall be present if the Area of Interest subscribed is a list of NR cell Ids. |
| globalRanNodeIdList | array(GlobalRanNodeId) | C | 1..N | Represents the list of NG RAN node identifiers that constitutes the area. This IE shall be present if the Area of Interest subscribed is a list of NG RAN node identifiers. |

#### 5.4.4.28 Type: GlobalRanNodeId

Table 5.4.4.28-1: Definition of type GlobalRanNodeId

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| plmnId | PlmnId | M | 1 | Indicates the identity of the PLMN that the RAN node belongs to. |
| n3IwfId | N3IwfId | C | 0..1 | This IE shall be included if the RAN node belongs to non 3GPP access (i.e a N3IWF).  (NOTE). |
| gNbId | GNbId | C | 0..1 | This IE shall be included if the RAN Node Id represents a gNB. When present, this IE shall contain the identifier of the gNB. (NOTE 1). |
| ngeNbId | NgeNbId | C | 0..1 | This IE shall be included if the RAN Node Id represents a NG-eNB. When present, this IE shall contain the identifier of an NG-eNB. (NOTE 1). |
| NOTE: At most one of the three attributes n3IwfId, gNbIdm, ngeNbId shall be present. | | | | |

#### 5.4.4.29 Type: GNbId

Table 5.4.4.29-1: Definition of type GNbId

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| bitLength | integer | M | 1 | Unsigned integer representing the bit length of the gNB ID as defined in clause 9.3.1.6 of 3GPP TS 38.413 [11], within the range 22 to 32 |
| gNbValue | string | M | 1 | This represents the identifier of the gNB.  The string shall be formatted with following pattern:  '^[A-Fa-f0-9]{6,8}$'  The value of the gNB ID shall be encoded in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The padding 0 shall be added to make multiple nibbles, the most significant character representing the padding 0 if required together with the 4 most significant bits of the gNB ID shall appear first in the string, and the character representing the 4 least significant bit of the gNB ID shall appear last in the string.  Examples:  A 30 bit value "382A3F47" indicates a gNB ID with value 0x382A3F47  A 22 bit value "2A3F47" indicates a gNB ID with value 0x2A3F47 |

#### 5.4.4.30 Type: PresenceInfoRm

This data type is defined in the same way as the "PresenceInfo" data type, but with the OpenAPI "nullable: true" property.

#### 5.4.4.31 Type: MaPduCapability

Table 5.4.4.31-1: Definition of type MaPduCapability

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| atsssLL | boolean | C | 0..1 | Indicates the ATSSS-LL capability.  true: Supported false (default): Not Supported |
| mptcp | boolean | C | 0..1 | Indicates the MPTCP capability.  true: Supported false (default): Not Supported |

#### 5.4.4.32 Type: AtsssCapability

Table 5.4.4.32-1: Definition of type AtsssCapability

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| atsssLL | boolean | C | 0..1 | Indicates the ATSSS-LL capability to support procedures related to Access Traffic Steering, Switching, Splitting (see clauses 4.2.10, 5.32 of 3GPP TS 23.501 [2]).  true: Supported false (default): Not Supported |
| mptcp | boolean | C | 0..1 | Indicates the MPTCP capability to support procedures related to Access Traffic Steering, Switching, Splitting (see clauses 4.2.10, 5.32 of 3GPP TS 23.501 [2]).  true: Supported false (default): Not Supported |

## 5.5 Data Types related to 5G QoS

### 5.5.1 Introduction

This clause defines common data types related to 5G QoS.

### 5.5.2 Simple Data Types

This clause specifies common simple data types.

Table 5.5.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
| Qfi | integer | Unsigned integer identifying a QoS flow, within the range 0 to 63. |
| QfiRm | integer | This data type is defined in the same way as the "Qfi" data type, but with the OpenAPI "nullable: true" property. |
| 5Qi | integer | Unsigned integer representing a 5G QoS Identifier (see clause 5.7.2.1 of 3GPP TS 23.501 [8]), within the range 0 to 255. |
| 5QiRm | integer | This data type is defined in the same way as the "5Qi" data type, but with the OpenAPI "nullable: true" property. |
| BitRate | string | String representing a bit rate that shall be formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$'  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps" |
| BitRateRm | string | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. |
| ArpPriorityLevel | integer | Unsigned integer indicating the ARP Priority Level (see clause 5.7.2.2 of 3GPP TS 23.501 [8]), within the range 1 to 15.  Values are ordered in decreasing order of priority, i.e. with 1 as the highest priority and 15 as the lowest priority. |
| ArpPriorityLevelRm | integer | This data type is defined in the same way as the "ArpPriorityLevel" data type, but with the OpenAPI "nullable: true" property. |
| 5QiPriorityLevel | integer | Unsigned integer indicating the 5QI Priority Level (see clauses 5.7.3.3 and 5.7.4 of 3GPP TS 23.501 [8]), within the range 1 to 127.  Values are ordered in decreasing order of priority, i.e. with 1 as the highest priority and 127 as the lowest priority. |
| 5QiPriorityLevelRm | integer | This data type is defined in the same way as the "5QiPriorityLevel" data type, but with the OpenAPI "nullable: true" property. |
| PacketDelBudget | Integer | Unsigned integer indicating Packet Delay Budget (see clauses 5.7.3.4 and 5.7.4 of 3GPP TS 23.501 [8])), expressed in milliseconds.  Minimum = 1. |
| PacketDelBudgetRm | integer | This data type is defined in the same way as the "PacketDelBudget" data type, but with the OpenAPI "nullable: true" property. |
| PacketErrRate | string | String representing Packet Error Rate (see clause 5.7.3.5 and 5.7.4 of 3GPP TS 23.501 [8]), expressed as a "*scalar* x 10-k" where the scalar and the *exponent k are each encoded as one decimal digit*..  Pattern: '^([0-9]E-[0-9])$'  Examples:  Packer Error Rate 4x10-6 shall be encoded as "4E-6".  Packer Error Rate 10-2 shall be encoded as "1E2". |
| PacketErrRateRm | string | This data type is defined in the same way as the "PacketErrRate" data type, but with the OpenAPI "nullable: true" property. |
| PacketLossRate | Integer | Unsigned integer indicating Packet Loss Rate (see clauses 5.7.2.8 and 5.7.4 of 3GPP TS 23.501 [8]), expressed in tenth of percent.  Minimum = 0. Maximum = 1000. |
| PacketLossRateRm | Integer | This data type is defined in the same way as the "PacketLossRate" data type, but with the OpenAPI "nullable: true" property. |
| AverWindow | Integer | Unsigned integer indicating Averaging Window (see clause 5.7.3.6 and 5.7.4 of 3GPP TS 23.501 [8]), expressed in milliseconds.  Minimum = 1. Maximum = 4095. Default = 2000.. |
| AverWindowRm | integer | This data type is defined in the same way as the "AverWindow" data type, but with the OpenAPI "nullable: true" property. |
| MaxDataBurstVol | Integer | Unsigned integer indicating Maximum Data Burst Volume (see clauses 5.7.3.7 and 5.7.4 of 3GPP TS 23.501 [8]), expressed in Bytes.  Minimum = 1. Maximum = 4095. |
| MaxDataBurstVolRm | Integer | This data type is defined in the same way as the "MaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. |
| SamplingRatio | Integer | Unsigned integer indicating Sampling Ratio (see clauses 4.15.1 of 3GPP TS 23.502 [28), expressed in percent.  Minimum = 1. Maximum = 100 |
| SamplingRatioRM | Integer | This data type is defined in the same way as the "SamplingRatio" data type, but with the OpenAPI "nullable: true" property. |

### 5.5.3 Enumerations

#### 5.5.3.1 Enumeration: PreemptionCapability

The enumeration PreemptionCapability indicates the pre-emption capability of a request on other QoS flows. See clause 5.7.2.2 of 3GPP TS 23.501 [8]. It shall comply with the provisions defined in table 5.5.3.1-1.

Table 5.5.3.1-1: Enumeration PreemptionCapability

|  |  |
| --- | --- |
| Enumeration value | Description |
| "NOT\_PREEMPT" | Shall not trigger pre-emption. |
| "MAY\_PREEMPT" | May trigger pre-emption. |

#### 5.5.3.2 Enumeration: PreemptionVulnerability

The enumeration PreemptionVulnerability indicates the pre-emption vulnerability of the QoS flow to pre-emption from other QoS flows. See clause 5.7.2.2 of 3GPP TS 23.501 [8]. It shall comply with the provisions defined in table 5.5.3.2-1.

Table 5.5.3.2-1: Enumeration PreemptionVulnerability

|  |  |
| --- | --- |
| Enumeration value | Description |
| "NOT\_PREEMPTABLE" | Shall not be pre-empted. |
| "PREEMPTABLE" | May be pre-empted. |

#### 5.5.3.3 Enumeration: ReflectiveQosAttribute

The enumeration ReflectiveQosAttribute indicates whether certain traffic of the QoS flow may be subject to Reflective QoS (see clause 5.7.2.3 of 3GPP TS 23.501 [2]). It shall comply with the provisions defined in table 5.5.3.3-1.

Table 5.5.3.3-1: Enumeration ReflectiveQosAttribute

|  |  |
| --- | --- |
| Enumeration value | Description |
| "RQOS" | Certain traffic of the Qos flow may be subject to Reflective QoS. |
| "NO\_RQOS" | Traffic of the Qos flow is not subject to Reflective QoS. |

#### 5.5.3.4 Void

#### 5.5.3.5 Enumeration: NotificationControl

The enumeration NotificationControl indicates whether notifications are requested from the RAN when the GFBR can no longer (or again) be fulfilled for a QoS Flow during the lifetime of the QoS Flow (see clause 5.7.2.4 of 3GPP TS 23.501 [2]). It shall comply with the provisions defined in table 5.5.3.5-1.

Table 5.5.3.5-1: Enumeration NotificationControl

|  |  |
| --- | --- |
| Enumeration value | Description |
| "REQUESTED" | Notifications are requested from the RAN. |
| "NOT\_REQUESTED" | Notifications are not requested from the RAN. |

#### 5.5.3.6 Enumeration: QosResourceType

The enumeration QosResourceType indicates whether a QoS Flow is non-GBR, delay critical GBR, or non-delay critical GBR (see clauses 5.7.3.4 and 5.7.3.5 of 3GPP TS 23.501 [2]). It shall comply with the provisions defined in table 5.5.3.6-1.

Table 5.5.3.6-1: Enumeration QosResourceType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "NON\_GBR" | Non-GBR QoS Flow. |
| "NON\_CRITICAL\_GBR" | Non-delay critical GBR QoS flow. |
| "CRITICAL\_GBR" | Delay critical GBR QoS flow. |

#### 5.5.3.7 Enumeration: PreemptionCapabilityRm

This enumeration is defined in the same way as the "PreemptionCapability" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.5.3.8 Enumeration: PreemptionVulnerabilityRm

This enumeration is defined in the same way as the "PreemptionVulnerability" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.5.3.9 Enumeration: ReflectiveQosAttributeRm

This enumeration is defined in the same way as the "ReflectiveQosAttribute" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.5.3.10 Enumeration: NotificationControlRm

This enumeration is defined in the same way as the "NotificationControl" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.5.3.11 Enumeration: QosResourceTypeRm

This enumeration is defined in the same way as the "QosResourceType" enumeration, but with the OpenAPI "nullable: true" property.

#### 5.5.3.12 Enumeration: AdditionalQosFlowInfo

The enumeration AdditionalQosFlowInfo provides additional QoS flow information (see clause 9.3.1.12 3GPP TS 38.413 [11]). It shall comply with the provisions defined in table 5.5.3.12-1.

Table 5.5.3.12-1: Enumeration AdditionalQosFlowInfo

|  |  |
| --- | --- |
| Enumeration value | Description |
| "MORE\_LIKELY" | Traffic for the QoS flow is likely to appear more often than traffic for other flows established for the PDU session. |

### 5.5.4 Structured Data Types

#### 5.5.4.1 Type: Arp

Table 5.5.4.1-1: Definition of type Arp

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| priorityLevel | ArpPriorityLevel | M | 1 | Defines the relative importance of a resource request. |
| preemptCap | PreemptionCapability | M | 1 | Defines whether a service data flow may get resources that were already assigned to another service data flow with a lower priority level. |
| preemptVuln | PreemptionVulnerability | M | 1 | Defines whether a service data flow may lose the resources assigned to it in order to admit a service data flow with higher priority level. |

#### 5.5.4.2 Type: Ambr

Table 5.5.4.2-1: Definition of type Ambr

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| uplink | BitRate | M | 1 | AMBR for uplink |
| downlink | BitRate | M | 1 | AMBR for downlink |

#### 5.5.4.3 Type: Dynamic5Qi

Table 5.5.4.3-1: Definition of type Dynamic5Qi

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| resourceType | QosResourceType | M | 1 | Defines the 5QI resource type. See clause 5.5.3.6. |  |
| priorityLevel | 5QiPriorityLevel | M | 1 | Defines the 5QI Priority Level. See clause 5.5.2. |  |
| packetDelayBudget | PacketDelBudget | M | 1 | Defines the packet delay budget. See clause 5.5.2. |  |
| packetErrRate | PacketErrRate | M | 1 | Defines the packet error rate. See clause 5.5.2. |  |
| averWindow | AverWindow | C | 0..1 | Defines the averaging window. See clause 5.5.2.  This IE shall be present only for a GBR QoS flow or a Delay Critical GBR QoS flow. |  |
| maxDataBurstVol | MaxDataBurstVol | C | 0..1 | Defines the maximum data burst volume. See clause 5.5.2.  This IE shall be present for a Delay Critical GBR QoS flow. |  |

#### 5.5.4.4 Type: NonDynamic5Qi

Table 5.5.4.4-1: Definition of type NonDynamic5Qi

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| priorityLevel | 5QiPriorityLevel | O | 0..1 | Defines the 5QI Priority Level. See clause 5.5.2.  When present, it contains the 5QI Priority Level value that overrides the standardized or pre-configured value. |  |
| averWindow | AverWindow | O | 0..1 | Defines the averaging window. See clause 5.5.2.  This IE may be present for a GBR QoS flow or a Delay Critical GBR QoS flow. When present, it contains the Averaging Window that overrides the standardized or pre-configured value. |  |
| maxDataBurstVol | MaxDataBurstVol | O | 0..1 | Defines the maximum data burst volume. See clause 5.5.2.  This IE may be present for a Delay Critical GBR QoS flow. When present, it contains the Maximum Data Burst Volume value that overrides the standardized or pre-configured value. |  |

#### 5.5.4.5 Type: ArpRm

This data type is defined in the same way as the "Arp" data type, but with the OpenAPI "nullable: true" property.

#### 5.5.4.6 Type: AmbrRm

This data type is defined in the same way as the "Ambr" data type, but with the OpenAPI "nullable: true" property.

## 5.6 Data Types related to 5G Trace

### 5.6.1 Introduction

This clause defines common data types related to 5G Trace.

### 5.6.2 Simple Data Types

This clause specifies common simple data types.

Table 5.6.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
|  |  |  |

### 5.6.3 Enumerations

#### 5.6.3.1 Enumeration: TraceDepth

The enumeration TraceDepth defines how detailed information should be recorded in the trace. See 3GPP TS 32.422 [19] for further description of the values. It shall comply with the provisions defined in table 5.6.3.1-1.

Table 5.6.3.1-1: Enumeration TraceDepth

|  |  |
| --- | --- |
| Enumeration value | Description |
| "MINIMUM" | Minimum |
| "MEDIUM" | Medium |
| "MAXIMUM" | Maximum |
| "MINIMUM\_WO\_VENDOR\_EXTENSION" | Minimum without vendor specific extension |
| "MEDIUM\_WO\_VENDOR\_EXTENSION" | Medium without vendor specific extension |
| "MAXIMUM\_WO\_VENDOR\_EXTENSION" | Maximum without vendor specific extension |

#### 5.6.3.2 Enumeration: TraceDepthRm

This enumeration is defined in the same way as the "TraceDepth" enumeration, but with the OpenAPI "nullable: true" property.

### 5.6.4 Structured Data Types

#### 5.6.4.1 Type: TraceData

Table 5.6.4.1-1: Definition of type TraceData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| traceRef | string | M | 1 | Trace Reference (see 3GPP TS 32.422 [19]).  It shall be encoded as the concatenation of MCC, MNC and Trace ID as follows:  <MCC><MNC>-<Trace ID>  The Trace ID shall be encoded as a 3 octet string in hexadecimal representation. Each character in the Trace ID string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the Trace ID shall appear first in the string, and the character representing the 4 least significant bit of the Trace ID shall appear last in the string.  Pattern: '^[0-9]{3}[0-9]{2,3}-[A-Fa-f0-9]{6}$' |
| traceDepth | TraceDepth | M | 1 | Trace Depth (see 3GPP TS 32.422 [19]). |
| neTypeList | string | M | 1 | List of NE Types (see 3GPP TS 32.422 [19]).  It shall be encoded as an octet string in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits shall appear first in the string, and the character representing the 4 least significant bit shall appear last in the string.  Octets shall be coded according to 3GPP TS 32.422 [19].  Pattern: '^[A-Fa-f0-9]+$' |
| eventList | string | M | 1 | Triggering events (see 3GPP TS 32.422 [19]).  It shall be encoded as an octet string in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits shall appear first in the string, and the character representing the 4 least significant bit shall appear last in the string.  Octets shall be coded according to 3GPP TS 32.422 [19].  Pattern: '^[A-Fa-f0-9]+$' |
| collectionEntityIpv4Addr | Ipv4Addr | C | 0..1 | IPv4 Address of the Trace Collection Entity (see 3GPP TS 32.422 [x).  At least one of the collectionEntityIpv4Addr or collectionEntityIpv6Addr attributes shall be present. |
| collectionEntityIpv6Addr | Ipv6Addr | C | 0..1 | IPv6 Address of the Trace Collection Entity (see 3GPP TS 32.422 [x).  At least one of the collectionEntityIpv4Addr or collectionEntityIpv6Addr attributes shall be present. |
| interfaceList | string | O | 0..1 | List of Interfaces (see 3GPP TS 32.422 [19]).  It shall be encoded as an octet string in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits shall appear first in the string, and the character representing the 4 least significant bit shall appear last in the string.  Octets shall be coded according to 3GPP TS 32.422 [19].  If this attribute is not present, all the interfaces applicable to the list of NE types indicated in the neTypeList attribute should be traced.  Pattern: '^[A-Fa-f0-9]+$' |

## 5.7 Data Types related to 5G Operator Determined Barring

### 5.7.1 Introduction

This clause defines common data types related to 5G Operator Determined Barring.

### 5.7.2 Simple Data Types

This clause specifies common simple data types.

Table 5.7.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
|  |  |  |

### 5.7.3 Enumerations

#### 5.7.3.1 Enumeration: RoamingOdb

The enumeration RoamingOdb defines the Barring of Roaming as. See 3GPP TS 23.015 [26] for further description. It shall comply with the provisions defined in table 5.7.3.1-1.

Table 5.7.3.1-1: Enumeration RoamingOdb

|  |  |
| --- | --- |
| Enumeration value | Description |
| "OUTSIDE\_HOME\_PLMN" | Barring of roaming outside the home PLMN |
| "OUTSIDE\_HOME\_PLMN\_COUNTRY" | Barring of roaming outside the home PLMN country |

#### 5.7.4.1 Enumeration: OdbPacketServices

The enumeration OdbPacketServices defines the Barring of Packet Oriented Services. See 3GPP TS 23.015 [26] for further description. It shall comply with the provisions defined in table 5.7.4.1-1.

Table 5.7.4.1-1: Enumeration OdbPacketServices

|  |  |
| --- | --- |
| Enumeration value | Description |
| "ALL\_PACKET\_SERVICES" | Barring of all Packet Oriented Services |
| "ROAMER\_ACCESS\_HPLMN\_AP" | Barring of Packet Oriented Services from access points that are within the HPLMN whilst the subscriber is roaming in a VPLMN |
| "ROAMER\_ACCESS\_VPLMN\_AP" | Barring of Packet Oriented Services from access points that are within the roamed to VPLMN. |

### 5.7.4 Structured Data Types

#### 5.7.4.1 Type: OdbData

Table 5.7.4.1-1: Definition of type OdbData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| roamingOdb | RoamingOdb | O | 0..1 | Barring of Roaming (see 3GPP TS 23.015 [26]). |

## 5.8 Data Types related to Charging

### 5.8.1 Introduction

This clause defines common data types related to Charging.

### 5.8.2 Simple Data Types

This clause specifies common simple data types.

Table 5.8.2-1: Simple Data Types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
| ChargingId | Uint32 | Charging identifier allowing correlation of charging information |
| RatingGroup | Uint32 | Identifier of a Rating Group |
| ServiceId | Uint32 | Identifier of a Service |

### 5.8.3 Enumerations

### 5.8.4 Structured Data Types

#### 5.8.4.1 Type: SecondaryRatUsageReport

Table 5.8.4.1-1: Definition of type SecondaryRatUsageReport

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| secondaryRatType | RatType | M | 1 | Secondary RAT type |
| qosFlowsUsageData | array(QosFlowUsageReport) | M | 1..N | QoS flows usage data |

#### 5.8.4.2 Type: QoSFlowUsageReport

Table 5.8.4.2-1: Definition of type QoSFlowUsageReport

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qfi | Qfi | M | 1 | QoS Flow Indicator |
| startTimeStamp | DateTime | M | 1 | UTC time indicating the start time of the collection period of the included usage data for DL and UL. |
| endTimeStamp | DateTime | M | 1 | UTC time indicating the end time of the collection period of the included usage data for DL and UL. |
| downlinkVolume | Int64 | M | 1 | Data usage for DL, encoding a number of octets |
| uplinkVolume | Int64 | M | 1 | Data usage for UL, encoding a number of octets |

#### 5.8.4.3 Type: SecondaryRatUsageInfo

Table 5.8.4.3-1: Definition of type SecondaryRatUsageInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| secondaryRatType | RatType | M | 1 | Secondary RAT type |
| qosFlowsUsageData | array(QosFlowUsageReport) | O | 1..N | QoS flows usage data |
| pduSessionUsageData | array(VolumeTimedReport) | O | 1..N | PDU session usage data |

#### 5.8.4.4 Type: VolumeTimedReport

Table 5.8.4.4-1: Definition of type VolumeTimedReport

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| startTimeStamp | DateTime | M | 1 | UTC time indicating the start time of the collection period of the included usage data for DL and UL. |
| endTimeStamp | DateTime | M | 1 | UTC time indicating the end time of the collection period of the included usage data for DL and UL. |
| downlinkVolume | Int64 | M | 1 | Data usage for DL, encoding a number of octets |
| uplinkVolume | Int64 | M | 1 | Data usage for UL, encoding a number of octets |

Annex A (normative):  
OpenAPI specification

## A.1 General

This Annex specifies the formal definition of common data types. It consists of an OpenAPI 3.0.0 specification, in YAML format.

This Annex takes precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API(s).

NOTE 1: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification files contained in this 3GPP Technical Specification are available on the public 3GPP file server in the following locations (see clause 5B of the 3GPP TR 21.900 [27] for further information):

- [https://www.3gpp.org/ftp/Specs/archive/OpenAPI/<Release>/](https://www.3gpp.org/ftp/Specs/archive/OpenAPI/%3cRelease%3e/), and

- [https://www.3gpp.org/ftp/Specs/<Plenary>/<Release>/OpenAPI/](https://www.3gpp.org/ftp/Specs/%3cPlenary%3e/%3cRelease%3e/OpenAPI/).

NOTE 2: To fetch the OpenAPI specification file after CT#83 plenary meeting for Release 15 in the above links <Plenary> must be replaced with the date the CT Plenary occurs, in the form of year-month (yyyy-mm), e.g. for CT#83 meeting <Plenary> must be replaced with value "2019-03" and <Release> must be replaced with value "Rel-15".

## A.2 Data related to Common Data Types

openapi: 3.0.0

info:

version: '1.2.0.alpha-1'

title: 'Common Data Types'

description: |

Common Data Types for Service Based Interfaces.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.571 Common Data Types for Service Based Interfaces, version 16.0.0 interim

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.571/'

paths: {}

components:

schemas:

#

# Common Data Types for Generic usage definitiones as defined in clause 5.2

#

#

# COMMON SIMPLE DATA TYPES

#

Binary:

format: binary

type: string

BinaryRm:

format: binary

type: string

nullable: true

Bytes:

format: byte

type: string

BytesRm:

format: byte

type: string

nullable: true

Date:

format: date

type: string

DateRm:

format: date

type: string

nullable: true

DateTime:

format: date-time

type: string

DateTimeRm:

format: date-time

type: string

nullable: true

DiameterIdentity:

type: string

pattern: '^([A-Za-z0-9]+([-A-Za-z0-9]+)\.)+[a-z]{2,}$'

DiameterIdentityRm:

type: string

pattern: '^([A-Za-z0-9]+([-A-Za-z0-9]+)\.)+[a-z]{2,}$'

nullable: true

Double:

format: double

type: number

DoubleRm:

format: double

type: number

nullable: true

DurationSec:

type: integer

DurationSecRm:

type: integer

nullable: true

Float:

format: float

type: number

FloatRm:

format: float

type: number

nullable: true

Int32:

format: int32

type: integer

Int32Rm:

format: int32

type: integer

nullable: true

Int64:

type: integer

format: int64

Int64Rm:

format: int64

type: integer

nullable: true

Ipv4Addr:

type: string

pattern: '^(([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])$'

example: '198.51.100.1'

Ipv4AddrRm:

type: string

pattern: '^(([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])$'

example: '198.51.100.1'

nullable: true

Ipv6Addr:

type: string

allOf:

- pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))$'

- pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))$'

example: '2001:db8:85a3::8a2e:370:7334'

Ipv6AddrRm:

type: string

allOf:

- pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))$'

- pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))$'

example: '2001:db8:85a3::8a2e:370:7334'

nullable: true

Ipv6Prefix:

type: string

allOf:

- pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))(\/(([0-9])|([0-9]{2})|(1[0-1][0-9])|(12[0-8])))$'

- pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))(\/.+)$'

example: '2001:db8:abcd:12::0/64'

Ipv6PrefixRm:

type: string

allOf:

- pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))(\/(([0-9])|([0-9]{2})|(1[0-1][0-9])|(12[0-8])))$'

- pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))(\/.+)$'

nullable: true

MacAddr48:

type: string

pattern: '^([0-9a-fA-F]{2})((-[0-9a-fA-F]{2}){5})$'

MacAddr48Rm:

type: string

pattern: '^([0-9a-fA-F]{2})((-[0-9a-fA-F]{2}){5})$'

nullable: true

SupportedFeatures:

type: string

pattern: '^[A-Fa-f0-9]\*$'

Uinteger:

type: integer

minimum: 0

UintegerRm:

type: integer

minimum: 0

nullable: true

Uint16:

type: integer

minimum: 0

maximum: 65535

Uint16Rm:

type: integer

minimum: 0

maximum: 65535

nullable: true

Uint32:

format: int32

type: integer

minimum: 0

Uint32Rm:

format: int32

type: integer

minimum: 0

nullable: true

Uint64:

format: int64

type: integer

minimum: 0

Uint64Rm:

format: int64

type: integer

minimum: 0

nullable: true

Uri:

type: string

UriRm:

type: string

nullable: true

VarUeId:

type: string

pattern: '^(imsi-[0-9]{5,15}|nai-.+|msisdn-[0-9]{5,15}|extid-[^@]+@[^@]+|.+)$'

VarUeIdRm:

type: string

pattern: '^(imsi-[0-9]{5,15}|nai-.+|msisdn-[0-9]{5,15}|extid-[^@]+@[^@]+|.+)$'

nullable: true

TimeZone:

type: string

TimeZoneRm:

type: string

nullable: true

#

# COMMON ENUMERATED DATA TYPES

#

PatchOperation:

anyOf:

- type: string

enum:

- add

- copy

- move

- remove

- replace

- test

- type: string

UriScheme:

anyOf:

- type: string

enum:

- http

- https

- type: string

ChangeType:

anyOf:

- type: string

enum:

- ADD

- MOVE

- REMOVE

- REPLACE

- type: string

#

# COMMON STRUCTURED DATA TYPES

#

ProblemDetails:

type: object

properties:

type:

$ref: '#/components/schemas/Uri'

title:

type: string

status:

type: integer

detail:

type: string

instance:

$ref: '#/components/schemas/Uri'

cause:

type: string

invalidParams:

type: array

items:

$ref: '#/components/schemas/InvalidParam'

minItems: 1

supportedFeatures:

$ref: '#/components/schemas/SupportedFeatures'

Link:

type: object

properties:

href:

$ref: '#/components/schemas/Uri'

LinkRm:

type: object

properties:

href:

$ref: '#/components/schemas/Uri'

nullable: true

PatchItem:

type: object

properties:

op:

$ref: '#/components/schemas/PatchOperation'

path:

type: string

from:

type: string

value:

nullable: true

required:

- op

- path

LinksValueSchema:

oneOf:

- type: array

items:

$ref: '#/components/schemas/Link'

minItems: 1

- $ref: '#/components/schemas/Link'

SelfLink:

type: object

properties:

self:

$ref: '#/components/schemas/Link'

required:

- self

InvalidParam:

type: object

properties:

param:

type: string

reason:

type: string

required:

- param

ChangeItem:

type: object

properties:

op:

$ref: '#/components/schemas/ChangeType'

path:

type: string

from:

type: string

origValue: {}

newValue: {}

required:

- op

- path

NotifyItem:

type: object

required:

- resourceId

- changes

properties:

resourceId:

$ref: '#/components/schemas/Uri'

changes:

type: array

items:

$ref: '#/components/schemas/ChangeItem'

minItems: 1

ComplexQuery:

oneOf:

- $ref: '#/components/schemas/Cnf'

- $ref: '#/components/schemas/Dnf'

Cnf:

type: object

required:

- cnfUnits

properties:

cnfUnits:

type: array

items:

$ref: '#/components/schemas/CnfUnit'

minItems: 1

Dnf:

type: object

required:

- dnfUnits

properties:

dnfUnits:

type: array

items:

$ref: '#/components/schemas/DnfUnit'

minItems: 1

CnfUnit:

type: object

required:

- cnfUnit

properties:

cnfUnit:

type: array

items:

$ref: '#/components/schemas/Atom'

minItems: 1

DnfUnit:

type: object

required:

- dnfUnit

properties:

dnfUnit:

type: array

items:

$ref: '#/components/schemas/Atom'

minItems: 1

Atom:

type: object

required:

- attr

- value

properties:

attr:

type: string

value: {}

negative:

type: boolean

NFDiscFactors:

type: object

properties:

targetNfType:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

requesterNfType:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

serviceNames:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

minItems: 1

uniqueItems: true

requesterNfInstanceFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

targetPlmnList:

type: array

items:

$ref: '#/components/schemas/PlmnId'

minItems: 1

requesterPlmnList:

type: array

items:

$ref: '#/components/schemas/PlmnId'

minItems: 1

targetNfInstanceId:

$ref: '#/components/schemas/NfInstanceId'

targetNfFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

hnrfUri:

$ref: '#/components/schemas/Uri'

snssais:

type: array

items:

$ref: '#/components/schemas/Snssai'

minItems: 1

plmnSpecificSnssaiList:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/PlmnSnssai'

minItems: 1

dnn:

$ref: '#/components/schemas/Dnn'

nsiList:

type: array

items:

type: string

minItems: 1

tai:

$ref: '#/components/schemas/Tai'

amfRegionId:

$ref: '#/components/schemas/AmfRegionId'

amfSetId:

$ref: '#/components/schemas/AmfSetId'

guami:

$ref: '#/components/schemas/Guami'

supi:

$ref: '#/components/schemas/Supi'

ueIpv4Address:

$ref: '#/components/schemas/Ipv4Addr'

ipDomain:

type: string

ueIpv6Prefix:

$ref: '#/components/schemas/Ipv6Prefix'

pgwInd:

type: boolean

pgw:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

gpsi:

$ref: '#/components/schemas/Gpsi'

externalGroupIdentity:

type: string

dataSet:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/DataSetId'

routingIndicator:

type: string

pattern: '^[0-9]{1,4}$'

groupIdList:

type: array

items:

$ref: '#/components/schemas/NfGroupId'

minItems: 1

dnaiList:

type: array

items:

$ref: '#/components/schemas/Dnai'

minItems: 1

pduSessionTypes:

type: array

items:

$ref: '#/components/schemas/PduSessionType'

minItems: 1

upfIwkEpsInd:

type: boolean

chfSupportedPlmn:

$ref: '#/components/schemas/PlmnId'

preferredLocality:

type: string

accessType:

$ref: '#/components/schemas/AccessType'

requiredFeatures:

type: array

items:

$ref: '#/components/schemas/SupportedFeatures'

minItems: 1

complexQuery:

$ref: '#/components/schemas/ComplexQuery'

#

# Data Types related to Subscription, Identification and Numbering as defined in clause 5.3

#

#

# SIMPLE DATA TYPES

#

Dnn:

type: string

DnnRm:

type: string

nullable: true

Gpsi:

type: string

pattern: '^(msisdn-[0-9]{5,15}|extid-[^@]+@[^@]+|.+)$'

GpsiRm:

type: string

pattern: '^(msisdn-[0-9]{5,15}|extid-[^@]+@[^@]+|.+)$'

nullable: true

GroupId:

type: string

pattern: '^[A-Fa-f0-9]{8}-[0-9]{3}-[0-9]{2,3}-([A-Fa-f0-9][A-Fa-f0-9]){1,10}$'

GroupIdRm:

type: string

pattern: '^[A-Fa-f0-9]{8}-[0-9]{3}-[0-9]{2,3}-([A-Fa-f0-9][A-Fa-f0-9]){1,10}$'

nullable: true

Pei:

type: string

pattern: '^(imei-[0-9]{15}|imeisv-[0-9]{16}|.+)$'

PeiRm:

type: string

pattern: '^(imei-[0-9]{15}|imeisv-[0-9]{16}|.+)$'

nullable: true

Supi:

type: string

pattern: '^(imsi-[0-9]{5,15}|nai-.+|.+)$'

SupiRm:

type: string

pattern: '^(imsi-[0-9]{5,15}|nai-.+|.+)$'

nullable: true

NfInstanceId:

type: string

format: uuid

AmfId:

type: string

pattern: '^[A-Fa-f0-9]{6}$'

AmfRegionId:

type: string

pattern: '^[A-Fa-f0-9]{2}$'

AmfSetId:

type: string

pattern: '^[0-3][A-Fa-f0-9]{2}$'

RfspIndex:

type: integer

minimum: 1

maximum: 256

RfspIndexRm:

type: integer

minimum: 1

maximum: 256

nullable: true

NfGroupId:

type: string

MtcProviderInformation:

type: string

#

# STRUCTURED DATA TYPES

#

Guami:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

amfId:

$ref: '#/components/schemas/AmfId'

required:

- plmnId

- amfId

GuamiRm:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

amfId:

$ref: '#/components/schemas/AmfId'

required:

- plmnId

- amfId

nullable: true

NetworkId:

type: object

properties:

mnc:

$ref: '#/components/schemas/Mnc'

mcc:

$ref: '#/components/schemas/Mcc'

#

# Data Types related to 5G Network as defined in clause 5.4

#

#

# SIMPLE DATA TYPES

#

ApplicationId:

type: string

ApplicationIdRm:

type: string

nullable: true

PduSessionId:

type: integer

minimum: 0

maximum: 255

Mcc:

type: string

pattern: '^\d{3}$'

MccRm:

type: string

pattern: '^\d{3}$'

nullable: true

Mnc:

type: string

pattern: '^\d{2,3}$'

MncRm:

type: string

pattern: '^\d{2,3}$'

nullable: true

Tac:

type: string

pattern: '(^[A-Fa-f0-9]{4}$)|(^[A-Fa-f0-9]{6}$)'

TacRm:

type: string

pattern: '(^[A-Fa-f0-9]{4}$)|(^[A-Fa-f0-9]{6}$)'

nullable: true

EutraCellId:

type: string

pattern: '^[A-Fa-f0-9]{7}$'

EutraCellIdRm:

type: string

pattern: '^[A-Fa-f0-9]{7}$'

nullable: true

NrCellId:

type: string

pattern: '^[A-Fa-f0-9]{9}$'

NrCellIdRm:

type: string

pattern: '^[A-Fa-f0-9]{9}$'

nullable: true

Dnai:

type: string

DnaiRm:

type: string

nullable: true

5GMmCause:

$ref: '#/components/schemas/Uinteger'

AmfName:

type: string

AreaCode:

type: string

AreaCodeRm:

type: string

nullable: true

N3IwfId:

type: string

pattern: '^[A-Fa-f0-9]+$'

NgeNbId:

type: string

pattern: '^(MacroNGeNB-[A-Fa-f0-9]{5}|LMacroNGeNB-[A-Fa-f0-9]{6}|SMacroNGeNB-[A-Fa-f0-9]{5})$'

#

# ENUMERATED DATA TYPES

#

AccessType:

type: string

enum:

- 3GPP\_ACCESS

- NON\_3GPP\_ACCESS

AccessTypeRm:

type: string

enum:

- 3GPP\_ACCESS

- NON\_3GPP\_ACCESS

nullable: true

RatType:

anyOf:

- type: string

enum:

- NR

- EUTRA

- WLAN

- VIRTUAL

- NBIOT

- type: string

RatTypeRm:

anyOf:

- type: string

enum:

- NR

- EUTRA

- WLAN

- VIRTUAL

- NBIOT

- type: string

nullable: true

PduSessionType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- IPV4V6

- UNSTRUCTURED

- ETHERNET

- type: string

PduSessionTypeRm:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- IPV4V6

- UNSTRUCTURED

- ETHERNET

- type: string

nullable: true

UpIntegrity:

anyOf:

- type: string

enum:

- REQUIRED

- PREFERRED

- NOT\_NEEDED

- type: string

UpIntegrityRm:

anyOf:

- type: string

enum:

- REQUIRED

- PREFERRED

- NOT\_NEEDED

- type: string

nullable: true

UpConfidentiality:

anyOf:

- type: string

enum:

- REQUIRED

- PREFERRED

- NOT\_NEEDED

- type: string

UpConfidentialityRm:

anyOf:

- type: string

enum:

- REQUIRED

- PREFERRED

- NOT\_NEEDED

- type: string

nullable: true

SscMode:

anyOf:

- type: string

enum:

- SSC\_MODE\_1

- SSC\_MODE\_2

- SSC\_MODE\_3

- type: string

SscModeRm:

anyOf:

- type: string

enum:

- SSC\_MODE\_1

- SSC\_MODE\_2

- SSC\_MODE\_3

- type: string

nullable: true

DnaiChangeType:

anyOf:

- type: string

enum:

- EARLY

- EARLY\_LATE

- LATE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- EARLY: Early notification of UP path reconfiguration.

- EARLY\_LATE: Early and late notification of UP path reconfiguration. This value shall only be present in the subscription to the DNAI change event.

- LATE: Late notification of UP path reconfiguration.

DnaiChangeTypeRm:

anyOf:

- type: string

enum:

- EARLY

- EARLY\_LATE

- LATE

- type: string

nullable: true

RestrictionType:

anyOf:

- type: string

enum:

- ALLOWED\_AREAS

- NOT\_ALLOWED\_AREAS

- type: string

RestrictionTypeRm:

anyOf:

- type: string

enum:

- ALLOWED\_AREAS

- NOT\_ALLOWED\_AREAS

- type: string

nullable: true

CoreNetworkType:

anyOf:

- type: string

enum:

- 5GC

- EPC

- type: string

CoreNetworkTypeRm:

anyOf:

- type: string

enum:

- 5GC

- EPC

- type: string

nullable: true

PresenceState:

anyOf:

- type: string

enum:

- IN\_AREA

- OUT\_OF\_AREA

- UNKNOWN

- INACTIVE

- type: string

#

# STRUCTURED DATA TYPES

#

Snssai:

type: object

properties:

sst:

type: integer

minimum: 0

maximum: 255

sd:

type: string

pattern: '^[A-Fa-f0-9]{6}$'

required:

- sst

PlmnId:

type: object

properties:

mcc:

$ref: '#/components/schemas/Mcc'

mnc:

$ref: '#/components/schemas/Mnc'

required:

- mcc

- mnc

PlmnIdRm:

type: object

properties:

mcc:

$ref: '#/components/schemas/Mcc'

mnc:

$ref: '#/components/schemas/Mnc'

required:

- mcc

- mnc

nullable: true

Tai:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

tac:

$ref: '#/components/schemas/Tac'

required:

- plmnId

- tac

TaiRm:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

tac:

$ref: '#/components/schemas/Tac'

required:

- plmnId

- tac

nullable: true

Ecgi:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

# PLMN Identity

eutraCellId:

$ref: '#/components/schemas/EutraCellId'

required:

- plmnId

- eutraCellId

EcgiRm:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

# PLMN Identity

eutraCellId:

$ref: '#/components/schemas/EutraCellId'

required:

- plmnId

- eutraCellId

nullable: true

Ncgi:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

nrCellId:

$ref: '#/components/schemas/NrCellId'

required:

- plmnId

- nrCellId

NcgiRm:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

nrCellId:

$ref: '#/components/schemas/NrCellId'

required:

- plmnId

- nrCellId

nullable: true

UserLocation:

type: object

properties:

eutraLocation:

$ref: '#/components/schemas/EutraLocation'

nrLocation:

$ref: '#/components/schemas/NrLocation'

n3gaLocation:

$ref: '#/components/schemas/N3gaLocation'

EutraLocation:

type: object

properties:

tai:

$ref: '#/components/schemas/Tai'

ecgi:

$ref: '#/components/schemas/Ecgi'

ageOfLocationInformation:

type: integer

minimum: 0

maximum: 32767

ueLocationTimestamp:

$ref: '#/components/schemas/DateTime'

geographicalInformation:

type: string

pattern: '^[0-9A-F]{16}$'

geodeticInformation:

type: string

pattern: '^[0-9A-F]{20}$'

globalNgenbId:

$ref: '#/components/schemas/GlobalRanNodeId'

required:

- tai

- ecgi

EutraLocationRm:

type: object

properties:

tai:

$ref: '#/components/schemas/Tai'

ecgi:

$ref: '#/components/schemas/Ecgi'

ageOfLocationInformation:

type: integer

minimum: 0

maximum: 32767

ueLocationTimestamp:

$ref: '#/components/schemas/DateTime'

geographicalInformation:

type: string

pattern: '^[0-9A-F]{16}$'

geodeticInformation:

type: string

pattern: '^[0-9A-F]{20}$'

globalNgenbId:

$ref: '#/components/schemas/GlobalRanNodeId'

required:

- tai

- ecgi

nullable: true

NrLocation:

type: object

properties:

tai:

$ref: '#/components/schemas/Tai'

ncgi:

$ref: '#/components/schemas/Ncgi'

ageOfLocationInformation:

type: integer

minimum: 0

maximum: 32767

ueLocationTimestamp:

$ref: '#/components/schemas/DateTime'

geographicalInformation:

type: string

pattern: '^[0-9A-F]{16}$'

geodeticInformation:

type: string

pattern: '^[0-9A-F]{20}$'

globalGnbId:

$ref: '#/components/schemas/GlobalRanNodeId'

required:

- tai

- ncgi

NrLocationRm:

type: object

properties:

tai:

$ref: '#/components/schemas/Tai'

ncgi:

$ref: '#/components/schemas/Ncgi'

ageOfLocationInformation:

type: integer

minimum: 0

maximum: 32767

ueLocationTimestamp:

$ref: '#/components/schemas/DateTime'

geographicalInformation:

type: string

pattern: '^[0-9A-F]{16}$'

geodeticInformation:

type: string

pattern: '^[0-9A-F]{20}$'

globalGnbId:

$ref: '#/components/schemas/GlobalRanNodeId'

required:

- tai

- ncgi

nullable: true

N3gaLocation:

type: object

properties:

n3gppTai:

$ref: '#/components/schemas/Tai'

n3IwfId:

type: string

pattern: '^[A-Fa-f0-9]+$'

ueIpv4Addr:

$ref: '#/components/schemas/Ipv4Addr'

ueIpv6Addr:

$ref: '#/components/schemas/Ipv6Addr'

portNumber:

$ref: '#/components/schemas/Uinteger'

UpSecurity:

type: object

properties:

upIntegr:

$ref: '#/components/schemas/UpIntegrity'

upConfid:

$ref: '#/components/schemas/UpConfidentiality'

required:

- upIntegr

- upConfid

UpSecurityRm:

type: object

properties:

upIntegr:

$ref: '#/components/schemas/UpIntegrity'

upConfid:

$ref: '#/components/schemas/UpConfidentiality'

required:

- upIntegr

- upConfid

nullable: true

NgApCause:

type: object

properties:

group:

$ref: '#/components/schemas/Uinteger'

value:

$ref: '#/components/schemas/Uinteger'

required:

- group

- value

BackupAmfInfo:

type: object

properties:

backupAmf:

$ref: '#/components/schemas/AmfName'

guamiList:

type: array

items:

$ref: '#/components/schemas/Guami'

minItems: 1

required:

- backupAmf

RefToBinaryData:

type: object

properties:

contentId:

type: string

required:

- contentId

RefToBinaryDataRm:

type: object

properties:

contentId:

type: string

required:

- contentId

nullable: true

RouteToLocation:

type: object

properties:

dnai:

$ref: '#/components/schemas/Dnai'

routeInfo:

$ref: '#/components/schemas/RouteInformation'

routeProfId:

type: string

nullable: true

required:

- dnai

anyOf:

- required: [ routeInfo ]

- required: [ routeProfId ]

nullable: true

RouteInformation:

type: object

properties:

ipv4Addr:

$ref: '#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: '#/components/schemas/Ipv6Addr'

portNumber:

$ref: '#/components/schemas/Uinteger'

required:

- portNumber

nullable: true

SubscribedDefaultQos:

type: object

required:

- 5qi

- arp

properties:

5qi:

$ref: '#/components/schemas/5Qi'

arp:

$ref: '#/components/schemas/Arp'

priorityLevel:

$ref: '#/components/schemas/5QiPriorityLevel'

Area:

type: object

oneOf:

- required:

- tacs

- required:

- areaCode

properties:

tacs:

type: array

items:

$ref: '#/components/schemas/Tac'

minItems: 1

areaCode:

$ref: '#/components/schemas/AreaCode'

ServiceAreaRestriction:

type: object

properties:

restrictionType:

$ref: '#/components/schemas/RestrictionType'

areas:

type: array

items:

$ref: '#/components/schemas/Area'

maxNumOfTAs:

$ref: '#/components/schemas/Uinteger'

maxNumOfTAsForNotAllowedAreas:

$ref: '#/components/schemas/Uinteger'

allOf:

#

# 1st condition: restrictionType and areas attributes shall be either both absent

# or both present

#

- oneOf:

- not:

required: [ restrictionType ]

- required: [ areas ]

#

# 2nd condition: if restrictionType takes value NOT\_ALLOWED\_AREAS,

# then maxNumOfTAs shall be absent

#

- anyOf:

- not:

required: [ restrictionType ]

properties:

restrictionType:

type: string

enum: [ NOT\_ALLOWED\_AREAS ]

- not:

required: [ maxNumOfTAs ]

#

# 3rd condition: if restrictionType takes value ALLOWED\_AREAS,

# then maxNumOfTAsForNotAllowedAreas shall be absent

#

- anyOf:

- not:

required: [ restrictionType ]

properties:

restrictionType:

type: string

enum: [ ALLOWED\_AREAS ]

- not:

required: [ maxNumOfTAsForNotAllowedAreas ]

PresenceInfo:

type: object

properties:

praId:

type: string

presenceState:

$ref: '#/components/schemas/PresenceState'

trackingAreaList:

type: array

items:

$ref: '#/components/schemas/Tai'

minItems: 1

ecgiList:

type: array

items:

$ref: '#/components/schemas/Ecgi'

minItems: 1

ncgiList:

type: array

items:

$ref: '#/components/schemas/Ncgi'

minItems: 1

globalRanNodeIdList:

type: array

items:

$ref: '#/components/schemas/GlobalRanNodeId'

minItems: 1

PresenceInfoRm:

type: object

properties:

praId:

type: string

presenceState:

$ref: '#/components/schemas/PresenceState'

trackingAreaList:

type: array

items:

$ref: '#/components/schemas/Tai'

minItems: 0

ecgiList:

type: array

items:

$ref: '#/components/schemas/Ecgi'

minItems: 0

ncgiList:

type: array

items:

$ref: '#/components/schemas/Ncgi'

minItems: 0

globalRanNodeIdList:

type: array

items:

$ref: '#/components/schemas/GlobalRanNodeId'

nullable: true

GlobalRanNodeId:

type: object

properties:

plmnId:

$ref: '#/components/schemas/PlmnId'

n3IwfId:

$ref: '#/components/schemas/N3IwfId'

gNbId:

$ref: '#/components/schemas/GNbId'

ngeNbId:

$ref: '#/components/schemas/NgeNbId'

oneOf:

- required: [ n3IwfId ]

- required: [ gNbId ]

- required: [ ngeNbId ]

required:

- plmnId

GNbId:

type: object

properties:

bitLength:

type: integer

minimum: 22

maximum: 32

gNBValue:

type: string

pattern: '^[A-Fa-f0-9]{6,8}$'

required:

- bitLength

- gNBValue

MaPduCapability:

type: object

properties:

atsssLL:

type: boolean

default: false

mptcp:

type: boolean

default: boolean

AtsssCapability:

type: object

properties:

atsssLL:

type: boolean

default: false

mptcp:

type: boolean

default: false

#

# Data Types related to 5G QoS as defined in clause 5.5

#

#

# SIMPLE DATA TYPES

#

#

Qfi:

type: integer

minimum: 0

maximum: 63

QfiRm:

type: integer

minimum: 0

maximum: 63

nullable: true

5Qi:

type: integer

minimum: 0

maximum: 255

5QiRm:

type: integer

minimum: 0

maximum: 255

nullable: true

BitRate:

type: string

pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$'

BitRateRm:

type: string

pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$'

nullable: true

ArpPriorityLevelRm:

type: integer

minimum: 1

maximum: 15

nullable: true

ArpPriorityLevel:

type: integer

minimum: 1

maximum: 15

nullable: true

description: nullable true shall not be used for this attribute

5QiPriorityLevel:

type: integer

minimum: 1

maximum: 127

5QiPriorityLevelRm:

type: integer

minimum: 1

maximum: 127

nullable: true

PacketDelBudget:

type: integer

minimum: 1

PacketDelBudgetRm:

type: integer

minimum: 1

nullable: true

PacketErrRate:

type: string

pattern: '^([0-9]E-[0-9])$'

PacketErrRateRm:

type: string

pattern: '^([0-9]E-[0-9])$'

nullable: true

PacketLossRate:

type: integer

minimum: 0

maximum: 1000

PacketLossRateRm:

type: integer

minimum: 0

maximum: 1000

nullable: true

AverWindow:

type: integer

minimum: 1

maximum: 4095

default: 2000

AverWindowRm:

type: integer

maximum: 4095

default: 2000

minimum: 1

nullable: true

MaxDataBurstVol:

type: integer

minimum: 1

maximum: 4095

MaxDataBurstVolRm:

type: integer

minimum: 1

maximum: 4095

nullable: true

SampleRatio:

type: integer

minimum: 1

maximum: 100

SampleRatioRm:

type: integer

minimum: 1

maximum: 100

nullable: true

#

# ENUMERATED DATA TYPES

#

PreemptionCapability:

anyOf:

- type: string

enum:

- NOT\_PREEMPT

- MAY\_PREEMPT

- type: string

PreemptionCapabilityRm:

anyOf:

- type: string

enum:

- NOT\_PREEMPT

- MAY\_PREEMPT

- type: string

nullable: true

PreemptionVulnerability:

anyOf:

- type: string

enum:

- NOT\_PREEMPTABLE

- PREEMPTABLE

- type: string

PreemptionVulnerabilityRm:

anyOf:

- type: string

enum:

- NOT\_PREEMPTABLE

- PREEMPTABLE

- type: string

nullable: true

ReflectiveQoSAttribute:

anyOf:

- type: string

enum:

- RQOS

- NO\_RQOS

- type: string

ReflectiveQoSAttributeRm:

anyOf:

- type: string

enum:

- RQOS

- NO\_RQOS

- type: string

nullable: true

NotificationControl:

anyOf:

- type: string

enum:

- REQUESTED

- NOT\_REQUESTED

- type: string

NotificationControlRm:

anyOf:

- type: string

enum:

- REQUESTED

- NOT\_REQUESTED

- type: string

nullable: true

QosResourceType:

anyOf:

- type: string

enum:

- NON\_GBR

- NON\_CRITICAL\_GBR

- CRITICAL\_GBR

- type: string

QosResourceTypeRm:

anyOf:

- type: string

enum:

- NON\_GBR

- NON\_CRITICAL\_GBR

- CRITICAL\_GBR

- type: string

nullable: true

AdditionalQosFlowInfo:

anyOf:

- type: string

enum:

- MORE\_LIKELY

- type: string

nullable: true

#

#

# STRUCTURED DATA TYPES

#

Arp:

type: object

properties:

priorityLevel:

$ref: '#/components/schemas/ArpPriorityLevel'

preemptCap:

$ref: '#/components/schemas/PreemptionCapability'

preemptVuln:

$ref: '#/components/schemas/PreemptionVulnerability'

required:

- priorityLevel

- preemptCap

- preemptVuln

ArpRm:

type: object

properties:

priorityLevel:

$ref: '#/components/schemas/ArpPriorityLevel'

preemptCap:

$ref: '#/components/schemas/PreemptionCapability'

preemptVuln:

$ref: '#/components/schemas/PreemptionVulnerability'

required:

- priorityLevel

- preemptCap

- preemptVuln

nullable: true

Ambr:

type: object

properties:

uplink:

$ref: '#/components/schemas/BitRate'

downlink:

$ref: '#/components/schemas/BitRate'

required:

- uplink

- downlink

AmbrRm:

type: object

properties:

uplink:

$ref: '#/components/schemas/BitRate'

downlink:

$ref: '#/components/schemas/BitRate'

required:

- uplink

- downlink

nullable: true

Dynamic5Qi:

type: object

properties:

resourceType:

$ref: '#/components/schemas/QosResourceType'

priorityLevel:

$ref: '#/components/schemas/5QiPriorityLevel'

packetDelayBudget:

$ref: '#/components/schemas/PacketDelBudget'

packetErrRate:

$ref: '#/components/schemas/PacketErrRate'

averWindow:

$ref: '#/components/schemas/AverWindow'

maxDataBurstVol:

$ref: '#/components/schemas/MaxDataBurstVol'

required:

- resourceType

- priorityLevel

- packetDelayBudget

- packetErrRate

NonDynamic5Qi:

type: object

properties:

priorityLevel:

$ref: '#/components/schemas/5QiPriorityLevel'

averWindow:

$ref: '#/components/schemas/AverWindow'

maxDataBurstVol:

$ref: '#/components/schemas/MaxDataBurstVol'

minProperties: 0

#

# Data Types related to 5G Trace as defined in clause 5.6

#

#

# SIMPLE DATA TYPES

#

#

#

# Enumerations

#

TraceDepth:

anyOf:

- type: string

enum:

- MINIMUM

- MEDIUM

- MAXIMUM

- MINIMUM\_WO\_VENDOR\_EXTENSION

- MEDIUM\_WO\_VENDOR\_EXTENSION

- MAXIMUM\_WO\_VENDOR\_EXTENSION

- type: string

TraceDepthRm:

anyOf:

- type: string

enum:

- MINIMUM

- MEDIUM

- MAXIMUM

- MINIMUM\_WO\_VENDOR\_EXTENSION

- MEDIUM\_WO\_VENDOR\_EXTENSION

- MAXIMUM\_WO\_VENDOR\_EXTENSION

- type: string

nullable: true

#

# STRUCTURED DATA TYPES

#

TraceData:

type: object

nullable: true

properties:

traceRef:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-[A-Fa-f0-9]{6}$'

traceDepth:

$ref: '#/components/schemas/TraceDepth'

neTypeList:

type: string

pattern: '^[A-Fa-f0-9]+$'

eventList:

type: string

pattern: '^[A-Fa-f0-9]+$'

collectionEntityIpv4Addr:

$ref: '#/components/schemas/Ipv4Addr'

collectionEntityIpv6Addr:

$ref: '#/components/schemas/Ipv6Addr'

interfaceList:

type: string

pattern: '^[A-Fa-f0-9]+$'

required:

- traceRef

- traceDepth

- neTypeList

- eventList

# Data Types related to 5G ODB as defined in clause 5.7

#

# SIMPLE DATA TYPES

#

#

#

# Enumerations

#

RoamingOdb:

anyOf:

- type: string

enum:

- OUTSIDE\_HOME\_PLMN

- OUTSIDE\_HOME\_PLMN\_COUNTRY

- type: string

OdbPacketServices:

anyOf:

- type: string

enum:

- ALL\_PACKET\_SERVICES

- ROAMER\_ACCESS\_HPLMN\_AP

- ROAMER\_ACCESS\_VPLMN\_AP

- type: string

nullable: true

#

# STRUCTURED DATA TYPES

#

OdbData:

type: object

properties:

roamingOdb:

$ref: '#/components/schemas/RoamingOdb'

#

# Data Types related to Charging as defined in clause 5.8

#

#

# SIMPLE DATA TYPES

#

#

ChargingId:

$ref: '#/components/schemas/Uint32'

RatingGroup:

$ref: '#/components/schemas/Uint32'

ServiceId:

$ref: '#/components/schemas/Uint32'

#

# Enumerations

#

#

# STRUCTURED DATA TYPES

#

SecondaryRatUsageReport:

type: object

properties:

secondaryRatType:

$ref: '#/components/schemas/RatType'

qosFlowsUsageData:

type: array

items:

$ref: '#/components/schemas/QosFlowUsageReport'

minItems: 1

required:

- secondaryRatType

- qosFlowsUsageData

QosFlowUsageReport:

type: object

properties:

qfi:

$ref: '#/components/schemas/Qfi'

startTimeStamp:

$ref: '#/components/schemas/DateTime'

endTimeStamp:

$ref: '#/components/schemas/DateTime'

downlinkVolume:

$ref: '#/components/schemas/Int64'

uplinkVolume:

$ref: '#/components/schemas/Int64'

required:

- qfi

- startTimeStamp

- endTimeStamp

- downlinkVolume

- uplinkVolume

SecondaryRatUsageInfo:

type: object

properties:

secondaryRatType:

$ref: '#/components/schemas/RatType'

qosFlowsUsageData:

type: array

items:

$ref: '#/components/schemas/QosFlowUsageReport'

minItems: 1

pduSessionUsageData:

type: array

items:

$ref: '#/components/schemas/VolumeTimedReport'

minItems: 1

required:

- secondaryRatType

VolumeTimedReport:

type: object

properties:

startTimeStamp:

$ref: '#/components/schemas/DateTime'

endTimeStamp:

$ref: '#/components/schemas/DateTime'

downlinkVolume:

$ref: '#/components/schemas/Int64'

uplinkVolume:

$ref: '#/components/schemas/Int64'

required:

- startTimeStamp

- endTimeStamp

- downlinkVolume

- uplinkVolume

#

# HTTP responses

#

responses:

'400':

description: Bad request

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'401':

description: Unauthorized

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'404':

description: Not Found

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'405':

description: Method Not Allowed

'408':

description: Request Timeout

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'406':

description: 406 Not Acceptable

'409':

description: Conflict

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'410':

description: Gone

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'411':

description: Length Required

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'412':

description: Precondition Failed

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'413':

description: Payload Too Large

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'414':

description: URI Too Long

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'415':

description: Unsupported Media Type

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'429':

description: Too Many Requests

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'500':

description: Internal Server Error

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'501':

description: Not Implemented

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'503':

description: Service Unavailable

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

'504':

description: Gateway Timeout

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetails'

default:

description: Generic Error

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-10 | CT4#80 | C4-175048 |  |  |  | Initial Draft. | 0.1.0 |
| 2017-10 | CT4#80 | C4-175400 |  |  |  | Skeleton and scope | 0.2.0 |
| 2017-12 | CT4#81 | C4-176442 |  |  |  | After CT4#81 | 0.3.0 |
| 2018-01 | CT4#82 | C4-181395 |  |  |  | After CT4#82 | 0.4.0 |
| 2018-03 | CT4#83 | C4-182440 |  |  |  | After CT4#83 | 0.5.0 |
| 2018-04 | CT4#84 | C4-183521 |  |  |  | After CT4#84 | 0.6.0 |
| 2018-05 | CT4#85 | C4-184635 |  |  |  | After CT4#85 | 0.7.0 |
| 2018-06 | CT#80 | CP-181110 |  |  |  | Presented for information and approval | 1.0.0 |
| 2018-06 | CT#80 |  |  |  |  | Approved in CT#80 | 15.0.0 |
| 2018-09 | CT#81 | CP-182065 | 0001 |  | F | ProblemDetails | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0002 |  | F | Structure of AmfId | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0012 |  | B | DNAI change notification type | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0015 |  | F | RatType | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0017 |  | B | Definition of DNAI | 15.1.0 |
| 2018-09 | CT#81 | CP-182068 | 0008 | 1 | B | Add support for 5G Trace | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0010 | 1 | F | OpenAPI Corrections | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0013 | 1 | B | Structure of ECGI and NCGI | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0007 | 1 | F | Averaging Window | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0020 | 1 | F | sd pattern | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0021 | 1 | F | Correction of the title of clauses 5.2.4.4 \_LinksValueSchema and 5.2.4.5 \_ SelfLink | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0023 |  | F | NAI format in 5G System | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0031 |  | F | GroupId Definition | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0009 | 1 | F | Removal of systematic references to the "format" keyword in data type definitions | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0033 |  | F | Naming Conventions | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0027 | 1 | F | 5GMMCause and NGAP Cause | 15.1.0 |
| 2018-09 | CT#81 | CP-182173 | 0006 | 3 | F | BackUp AMF Info | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0035 |  | F | URI Scheme | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0024 | 2 | F | Cleanup of the specification | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0025 | 1 | F | Correction to Regular Expression Pattern of GPSI | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0005 | 4 | F | Common data types: NonDynamic5qi and Dynamic5qi | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0028 | 1 | F | Common data type used in both TS 29.505 and TS 29.519 | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0029 | 1 | B | n6 Traffic Routing Information data type | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0019 | 4 | F | DefaultQosInformation | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0034 | 1 | F | Update of N3gaLocation data type | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0016 | 3 | F | Mobility Restriction | 15.1.0 |
| 2018-09 | CT#81 | CP-182042 | 0030 | 3 | F | Adding "nullable" property to OpenAPI definitions of data types | 15.1.0 |
| 2018-09 | CT#81 | CP-182174 | 0026 | 3 | F | Presence Reporting Area | 15.1.0 |
| 2018-09 | CT#81 | CP-182011 | 0032 | 4 | F | Adding age of location, geographic information and other missing ones in the UserLocation type | 15.1.0 |
| 2018-09 | CT#81 | CP-182183 | 0036 | 1 | B | Common data type for data change notification | 15.1.0 |
| 2018-09 | CT#81 | CP-182065 | 0037 |  | F | API version number update | 15.1.0 |
| 2018-12 | CT#82 | CP-183024 | 0040 |  | F | Application ID | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0049 |  | F | Corrections to PDU Session Id, PDU Session Type and SupportedFeatures | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0038 | 1 | F | Area definition | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0047 | 1 | F | DNN | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0044 | 1 | F | Update of missing status code 429 in TS 29.571 | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0057 | 1 | F | 29571 CR cardinality | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0045 | 2 | F | The ARP in Default QoS | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0058 | 1 | F | Snssai pattern | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0039 | 1 | F | GroupId pattern | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0059 |  | F | Adding of HTTP status code "406 Not Acceptable" | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0041 | 1 | F | VarUeId definition | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0061 |  | F | ProblemDetails for 501 | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0063 |  | F | ChangeItem alignment | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0046 | 2 | F | Regular Expression Patterns | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0048 | 3 | F | Alignments with NGAP | 15.2.0 |
| 2018-12 | CT#82 | CP-183168 | 0065 | 1 | F | Secondary RAT usage data reporting | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0060 | 1 | F | Data types associated with Subscribed and Authorized Default QoS for Default QoS Flow | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0042 | 3 | F | Alignment of pattern for data types with "nullable" property | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0062 | 1 | F | NF Group Id | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0053 | 2 | F | data type for complex query expression | 15.2.0 |
| 2018-12 | CT#82 | CP-183161 | 0064 | 2 | F | NgRanIdentifier and PresenceInfo | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0068 |  | F | Addition of HTTP status code "412 Precondition Failed" | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0051 | 3 | F | Introduction of Barring of Roaming in 5GC | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0066 | 1 | F | Service Area Restriction | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0067 | 1 | F | Charging related types | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0070 |  | F | Correction of the reference for the SupportedFeatures Data Type | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0072 | 1 | F | Update open API version | 15.2.0 |
| 2018-12 | CT#82 | CP-183024 | 0073 |  | F | ExternalDoc update | 15.2.0 |
| 2019-03 | CT#83 | CP-190029 | 0075 | 3 | F | Corrections on subscribed Priority | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0076 | 1 | F | AmfRegionId and AmfSetId | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0077 | 2 | F | Supported features | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0078 | 2 | F | Corrections on n3iwf Id | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0079 | 2 | F | Corrections on the encoding of bit string | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0081 | 2 | F | Corrections on Type RouteToLocation | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0082 | 1 | F | ODB correction | 15.3.0 |
| 2019-03 | CT#83 | CP-190029 | 0083 |  | F | 3GPP TS 29.571 API version update | 15.3.0 |
| 2019-06 | CT#84 | CP-191041 | 0077 | 3 | F | CR not implemented – Supported Features | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0084 | 1 | F | Service Area Restriction | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0087 | 1 | F | ChangeItem Indicating Complete Resource Creation or Removal | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0089 | 2 | F |  | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0090 | 1 | F | Clarificaiton on Universal Matching Pattern Schema | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0086 | 2 | F | Correct the discription of 5qi in SubscribedDefaultQos | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0097 |  | F | AreaCode | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0094 | 1 | F | Required attributes in NotifyItem | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0095 | 1 | F | Regular Expression Pattern of DiameterIdentity | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0096 | 1 | F | Secondary RAT Usage reporting at PDU session level | 15.4.0 |
| 2019-06 | CT#84 | CP-191041 | 0099 | 2 | F | Copyright Note in YAML file | 15.4.0 |
| 2019-06 | CT#84 | CP-191048 | 0100 | 1 | B | 3GPP TS 29.571 API version update | 16.0.0 |
| 2019-06 | CT#84 | CP-191050 | 0093 |  | B | Definition of MTC provider Information | 16.0.0 |
| 2019-06 | CT#84 | CP-191050 | 0098 | 1 | B | Extend value of RAT Type to add NBIOT | 16.0.0 |
| 2019-06 | CT#84 | CP-191051 | 0088 | 3 | B | Common Data Type for ATSSS Capability | 16.0.0 |
| 2019-06 | CT#84 | CP-191052 | 0085 | 1 | B | Addition of Event Reporting Information Parameters for network data analytics | 16.0.0 |
| 2019-06 | CT#84 | CP-191055 | 0091 | 2 | B | NF discovery factors | 16.0.0 |